**REQUEST FOR QUOTATION  
SPECIFICATION OF GOODS**

**Procurement No:** **09-G001-23**

## Specification

### Background

Toward end of last year 2022, disaster and risk management unit (DRMU) has planned to tender out construction materials for 6 disaster projects as the first lot to be executed into the procurement process and implemented hopefully early beginning of the next year. These projects are initiated from outer islands, and the plan to complete the procurement process for this lot is to be within the first quarter of this year.

**Objectives**

This project will target to repair what disaster interferences are and provide comfort zone to those who are hardly to live due to the impacts of disaster.

Communities will be targeted to live in and maintain their social entertainment in a more comfort zone

### Requirements

All supporting documentation must be in English.

should provide a clear quote(s) and follow every instruction stated in this template starting from submission to delivering of goods.

The following below listed documents should be provided

1. Business Registration with nature of business indication that the tenderer is capable to do hardware supplies. Failure to provide such registration will result in disqualification of the tenderer
2. Signed certificate for compliance form should be provided. (Failure will result in disqualifying the tenderer)
3. Tax clearance letter from Tax Office for tax registered companies (Failure to provide will result in rejection of the tender)
4. A complete quotation for financial component of the proposal
5. A complete technical requirement in achieving the specifications of goods indicated in this “Specification template”

### Installation services

Work implementation must be started upon the arrival of construction materials at site.

### Delivery Time

Tenderers are required to provide their time schedule for delivery of these construction materials to their different respective sites. Tenderers should also indicate goods available on hand and goods to be imported from overseas and the time frame for ordering of goods.

## Description of the Goods

1. **Construction of Rawannawi seawall, Marakei**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Material list - Construction of KUC Rawannawi seawall (Marakei)** | | |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| 1 | Portland Cements | 850 | bag |  |  |
| 2 | Geotextile 100m/roll | 1 | roll |  |  |
| 3 | Sandbag | 1300 | pcs |  |  |
| 4 | Formply sheet 3/4" | 7 | sheets |  |  |
| 5 | Timber frame 100x50mm | 12 | lengths |  |  |
| 6 | Nails 4" | 7 | kg |  |  |
| 7 | Nails 3" | 4 | kg |  |  |
| 8 | Nails flat 1 1/2 | 4 | kg |  |  |
| 9 | PVC Pipe 100mm | 2 | lengths |  |  |
| 10 | hand saw | 1 | nos |  |  |
| 11 | Tape measure 50mtr | 1 | nos |  |  |
| 12 | Tape measure 8mtr | 1 | nos |  |  |
| 13 | Bench bar | 1 | nos |  |  |
| 14 | shovels | 11 | pcs |  |  |
| 15 | hammers | 1 | pcs |  |  |
| 16 | wheel barrow | 3 | nos |  |  |
| 17 | crow bar | 1 | pcs |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |

1. **Rehab for KUC Tabomatang maneaba, Nikunau**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Materia list - Rehab for KUC Tabomatang maneaba (Nikunau)** | |  |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
|  | **Concrete works** |  |  |  |  |
| 1 | Cement 40kg | 2 | bags |  |  |
| 2 | 125mm x 12mm dia dynabolt | 12 | no |  |  |
| 3 | 175mm x 12mm dia galvanised bolt complete | 24 | no |  |  |
| 4 | 250x12mm diameter bolt with nut & 2 washers | 6 | no. |  |  |
|  | **Metal work** |  |  |  |  |
| 5 | 150mm dia galv pipe | 3 | length |  |  |
| 6 | 2400x1200x10mm metal plate sheet | 1 | sheets |  |  |
|  | **Carpentry** |  |  |  |  |
| 7 | Radiata pine 200x50mm in 6m long to be dressed | 32 | length |  |  |
| 8 | Plywood 2400x1200x4.5mm thick for gusset 8 | 8 | sht |  |  |
| 9 | Bracing Straps 'pryda' 25x1.0mm galv. Steel or mitek 30x0.8 galv steel strap. | 8 | roll |  |  |
| 10 | 100x50mm timber pine in 6m long | 54 | leng |  |  |
| 11 | 100x50mm timber pine in 6m long | 13 | leng |  |  |
| 12 | Radiata pine 75x50mm in 6m long to be dressed | 91 | length |  |  |
|  | *Fascia board* |  |  |  |  |
| 13 | 200x25mm timber pine | 15 | leng |  |  |
| 14 | 200x25mm timber pine | 4 | leng |  |  |
| 15 | Marine plywood 12mm for gable lining | 7 | sht |  |  |
|  | **Roofing** |  |  |  |  |
| 16 | 8ft corrugated roof zincalume above long rafters | 51 | sheets |  |  |
| 17 | 10ft corrugated roof zincalume | 51 | sheets |  |  |
| 18 | 19ft corrugated roof zincalume | 51 | sheets |  |  |
| 19 | 15ft corrugated roof zincalume | 25 | sheets |  |  |
| 20 | 12ft corrugated roof zincalume | 21 | sheets |  |  |
| 21 | 8ft corrugated roof zincalume for hips | 28 | sheets |  |  |
| 22 | Aluminium ridge cap 8'' | 8 | sheets |  |  |
| 23 | Flashing 8'0" | 12 | pcs |  |  |
|  | **Painting and decoration** |  |  |  |  |
| 24 | Oil base undercoat @ 4liters/tin | 5 | tn |  |  |
| 25 | Semi-gloss enamel @ 4liters/tin | 10 | tn |  |  |
| 26 | High gloss enamel paint @ 4liters/tin | 10 | tn |  |  |
| 27 | Tray Paint | 3 | no |  |  |
| 28 | 3 inch paint brush | 5 | no |  |  |
| 29 | 2 inch paint brush | 5 | no |  |  |
|  | **Nails** |  |  |  |  |
| 30 | 2 1/2" twisted roofing nail complete with rubber washers | 37 | kg |  |  |
| 31 | 2" galvanised nail flat head | 6 | kg |  |  |
| 32 | 3 inch galv. Nail | 21 | kg |  |  |
| 33 | 4" galvanised nail | 54 | kg |  |  |
| 34 | 2'' clout nail for gusset | 2 | kg |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |

1. **Rehab for Ueen Te Aireti maneaba, Onotoa**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Materia list - Rehab for KUC Ueen Te Aireti Maneaba (Onotoa)** | |  |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
|  | **Concrete work (Cements type GP or GB and to be 20MPA Concrete Strength)** |  |  |  |  |
| 1 | Portland cement 40kg | 70 | bags |  |  |
| 2 | Polythene damp proof membrane (60mx2m wide) 0.2mm thick | 1 | roll |  |  |
| 3 | Tie wire | 1 | roll |  |  |
|  | **Formwork** |  |  |  |  |
| 4 | Formply 3/4" thick | 2 | sheet |  |  |
| 5 | 50x50mm timber pine in 6m long | 5 | length |  |  |
|  | **Bar Reinforcement** |  |  |  |  |
| 6 | D20mm dia reinforcing bar | 31 | length |  |  |
| 7 | D12mm dia reinforcing steel (6m length) | 13 | length |  |  |
| 8 | Reinforcing mesh SL 102 size: 6mx2.4m wide | 3 | sheet |  |  |
|  | **Metal Work** |  |  |  |  |
| 9 | 120x150x10mm thick angle iron plate | 12 | no |  |  |
| 10 | 16mm dia galvanized bolts complete with nuts and washers 120mm long | 32 | no |  |  |
|  | **Structural timber pine (Treated pine timber)** |  |  |  |  |
| 11 | Timber pine 200z50mm in 6m long to be dressed | 12 | length |  |  |
| 12 | Timber pine 200x25mm in 6m long fascia and barge | 8 | length |  |  |
| 13 | Timber pine 100x50mm in 6m long to be dressed | 25 | length |  |  |
| 14 | Timber pine 75x50mm in 6m long to be dressed | 26 | length |  |  |
| 15 | Ex 150x25 radiant pine in 6m long | 15 | length |  |  |
| 16 | 12mm thick plywood gable lining | 4 | sheet |  |  |
|  | **Roofing Materials** |  |  |  |  |
| 17 | 0.55mm BMT colorbond 8feet 2.44m ` | 32 | sheet |  |  |
| 18 | 0.55mm BMT colorbond 9feet 2.56m | 22 | sheet |  |  |
| 19 | 0.55mm BMT colorbond ridge capping | 3 | pcs |  |  |
| 20 | 0.55mm BMT colorbond roof flashing | 6 | sheet |  |  |
| 21 | 0.55mm BMT colorbond eaves guttering with bracket 8ft | 14 | pcs |  |  |
| 22 | stop ends | 2 | no |  |  |
| 23 | outlet to gutter | 2 | no |  |  |
| 24 | 100mm diameter upvc downpipe including clips (6m long) | 12 | length |  |  |
| 25 | 100mm diameter bend | 2 | no |  |  |
| 26 | 100mm diameter tee | 1 | no |  |  |
| 27 | hydroseal | 1 | tin |  |  |
| 28 | silicone | 1 | tube |  |  |
| 29 | Rivert (100no/pkt) | 1 | pkt |  |  |
|  | **Painting and Decorating** |  |  |  |  |
| 30 | Acrylic primer sealer undercoat 4ltr | 3 | tin |  |  |
| 31 | H/gloss 4ltrs | 3 | tin |  |  |
| 32 | Undercoat 4ltrs | 3 | tin |  |  |
| 33 | acrylic paint 4ltrs | 2 | tin |  |  |
| 34 | Tray complete with roller and sleeve | 2 | no |  |  |
| 35 | 4 inch paint brush | 2 | no |  |  |
| 36 | 2 inch paint brush | 2 | no |  |  |
| 37 | 1 inch paint brush | 2 | no |  |  |
|  | **Electrical** |  |  |  |  |
| 38 | 4'0 fluorescent light fittings single tube complete | 2 | no |  |  |
| 39 | General power outlet double complete | 2 | no |  |  |
| 40 | light switch one way | 1 | no |  |  |
| 41 | 1.5mm cable 3 core | 10 | mtr |  |  |
| 42 | 2.5mm cable 3 core | 10 | mtr |  |  |
| 43 | 6mm cable | 10 | mtr |  |  |
| 44 | Earth wire 4mm cable | 10 | mtr |  |  |
| 45 | 25mm pvc pipe conduit | 12 | length |  |  |
| 46 | Switchboard box for 6 circuit breaker | 1 | no |  |  |
| 47 | 10amp circuit breaker | 1 | no |  |  |
| 48 | 20amp circuit breaker | 1 | no |  |  |
| 49 | 60amp circuit breakder | 1 | no |  |  |
| 50 | insulating tape | 1 | no |  |  |
|  | **Nails, Screw Bolt** |  |  |  |  |
| 51 | 4 inch nail | 10 | pkt |  |  |
| 52 | 3 inch nail | 10 | pkt |  |  |
| 53 | 2 inch nail | 10 | pkt |  |  |
| 54 | Hexagon roofing screw with EPDM washers | 10 | kg |  |  |
|  | **External works** |  |  |  |  |
| 55 | 6000ltrs water tank completed with outlet | 1 | no |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |

1. **Rehab for Catholic Otowae Parish maneaba, Onotoa**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Materia list - Rehab for Otowae Catholic Parish maneaba (Onotoa)** | |  |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
|  | **Concrete work (Cements type GP or GB and to be 20MPA Concrete Strength)** |  |  |  |  |
| 1 | Portland cement 40kg | 1219 | bags |  |  |
| 2 | Polythene damp proof membrane (60mx2m wide) 0.2mm thick | 24 | roll |  |  |
| 3 | Tie wire (15mtrs) | 23 | coil |  |  |
|  | **Formwork** |  |  |  |  |
| 4 | Formply 3/4" thick | 72 | sheet |  |  |
| 5 | 100x50mm timber pine in 6m long | 172 | length |  |  |
| 6 | 50x50mm timber pine in 6m long | 285 | length |  |  |
|  | **Bar Reinforcement** |  |  |  |  |
| 7 | D20mm dia reinforcing steel (6m length) deform | 65 | length |  |  |
| 8 | D12mm dia reinforcing steel (6m length) deform | 89 | length |  |  |
| 9 | D10mm dia reinforcing steel (6m length) deform | 159 | length |  |  |
| 10 | D6mm dia reinforcing steel (6m length)smooth | 27 | length |  |  |
| 11 | Reinforcing mesh SL 102 size: 6mx2.4m wide | 43 | sheet |  |  |
|  | **Metal Work** |  |  |  |  |
| 12 | Galvanized pipe (150mm) | 4 | no |  |  |
| 13 | galvanized pipe 50mm | 10 | length |  |  |
| 14 | costom bracket | 28 | no |  |  |
|  | **Structural timber pine (Treated pine timber)** |  |  |  |  |
| 15 | Timber pine 300x300mm in 6m long to be dressed 150c50mm laminated timber | 118.4 | length |  |  |
| 16 | Timber pine 250x100mm in 6m long to be dressed | 20 | length |  |  |
| 17 | Timber pine 250x50mm in 6m long to be dressed | 137 | length |  |  |
| 18 | Timber pine 200x25mm in 6m long to be dressed | 24 | length |  |  |
| 19 | Timber pine 150x50mm in 6m long to be dressed | 25 | length |  |  |
| 20 | Timber pine 75x50mm in 6m long to be dressed | 130 | length |  |  |
|  | **Roofing Materials** |  |  |  |  |
| 21 | 0.55mm BMT colorbond 19feet 5.80m ` | 42 | sheet |  |  |
| 22 | 0.55mm BMT colorbond 15feet 4.58m | 188 | sheet |  |  |
| 23 | 0.55mm BMT colorbond 11feet 3.36m | 90 | sheet |  |  |
| 24 | 0.55mm BMT colorbond 9feet 2.75m | 27 | sheet |  |  |
| 25 | 0.55mm BMT colorbond 2.14m | 12 | sheet |  |  |
| 26 | 0.55mm BMT colorbond 1.83m | 12 | sheet |  |  |
| 27 | syslation 20x1.5m | 66 | roll |  |  |
| 28 | 0.55mm BMT colorbond ridge capping | 18 | pcs |  |  |
| 29 | 0.55mm BMT colorbond roof flashing | 12 | pcs |  |  |
| 30 | Gutter 2.4m | 41 | no |  |  |
| 31 | External mitre Gutter | 4 | no |  |  |
| 32 | Outlet to gutter | 2 | no |  |  |
| 33 | 100mm diameter upvc downpipe in 6m long | 6 | length |  |  |
| 34 | 100mm diameter bend | 12 | no |  |  |
| 35 | 100mm diameter tee | 3 | no |  |  |
|  | **Lining** |  |  |  |  |
| 36 | Plywood 12mm | 14 | sheet |  |  |
|  | **Painting and Decorating** |  |  |  |  |
| 37 | undercoat enamel 4ltrs | 7 | tin |  |  |
| 38 | semi gloss 4ltrs | 7 | tin |  |  |
| 39 | semi gloss 100% white | 3 | tin |  |  |
| 40 | hulux acrylic sealer 4ltrs | 3 | tin |  |  |
| 41 | roller brush 9" + tray | 4 | no |  |  |
| 42 | roller brush 4" + tray | 4 | no |  |  |
| 43 | 4 inch paint brush | 4 | no |  |  |
| 44 | 3 inch paint brush | 3 | no |  |  |
| 45 | roller brush 9" | 4 | no |  |  |
| 46 | mouse roller | 4 | no |  |  |
| 47 | wood putty | 1 | kg |  |  |
| 48 | Turbentine @4.5ltrs/galon | 3 | galon |  |  |
| 49 | Silicone tube | 3 | tube |  |  |
| 50 | silicone gun | 1 | no |  |  |
|  | **Electrical** |  |  |  |  |
| 51 | 4'0 led light fittings single tube complete | 16 | no |  |  |
| 52 | pandant light | 4 | no |  |  |
| 53 | light switch one way | 3 | no |  |  |
| 54 | Earth wire 4mm cable | 5 | mtr |  |  |
| 55 | Switchboard complete with circuit breakers, wiring and connections and other associated components | 1 | sum |  |  |
|  | **Glues** |  |  |  |  |
| 56 | Epoxy glue 1ltr | 1 | tin |  |  |
|  | **Nails, Screw Bolt** |  |  |  |  |
| 57 | Total cost (vat inclusive) | 55 | pkt |  |  |
| 58 | 3" galvanized @ 100pcs/pkt | 55 | pkt |  |  |
| 59 | 2"x3.15mm bullet head galvanized nails @ 100pcs/pkt | 20 | pkt |  |  |
| 60 | M16 galvanized bolt 200mm length | 224 | no |  |  |
| 61 | M16 galvanized bolt 400mm length | 96 | no |  |  |
| 62 | M12 galvanized bolt 150mm length | 112 | no |  |  |
| 63 | M12 galvanized bolt 200mm length | 140 | no |  |  |
| 64 | Wood screw 2" | 20 | pkt |  |  |
| 65 | Wood screw 3" | 20 | pkt |  |  |
| 66 | Roofing nails 3" | 30 | pkt |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction of Raorao seawall, Onotoa**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Material list - Construction of Raorao seawall, Onotoa** | | |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| 1 | Portland Cements | 1500 | bag |  |  |
| 2 | Geotextile 100m/roll | 1 | roll |  |  |
| 3 | Sandbag | 2300 | pcs |  |  |
| 4 | Formply sheet 3/4" | 17 | sheets |  |  |
| 5 | Timber frame 100x50mm | 30 | lengths |  |  |
| 6 | Nails 4" | 10 | kg |  |  |
| 7 | Nails 3" | 3 | kg |  |  |
| 8 | Nails flat 1 1/2 | 3 | kg |  |  |
| 9 | PVC Pipe 100mm | 2 | lengths |  |  |
| 10 | hand saw | 1 | nos |  |  |
| 11 | Tape measure 50mtr | 1 | nos |  |  |
| 12 | Tape measure 8mtr | 1 | nos |  |  |
| 13 | Bench bar | 2 | nos |  |  |
| 14 | shovels | 30 | pcs |  |  |
| 15 | hammers | 2 | pcs |  |  |
| 16 | wheel barrow | 4 | nos |  |  |
| 17 | crow bar | 2 | pcs |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |

1. **Rehab for KUC Tabuarorae maneaba, Onotoa**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Materia list - Rehab for KUC Tabuarorae Church (Onotoa)** | |  |  |  |  |
| **item #** | **Description** | **Qty** | **Unit** | **Price Quotation** | **T/Price Quotation** |
|  | **Concrete work (Cements type GP or GB and to be 20MPA Concrete Strength)** |  |  |  |  |
| 1 | Portland cement 40kg | 100 | bags |  |  |
|  | **Formwork** |  |  |  |  |
| 2 | Formply 3/4" thick | 19 | sheet |  |  |
| 3 | D12mm dia reinforcing steeel ( in 6m length) deform | 13 | length |  |  |
| 4 | Welding machine charge | 5 | no |  |  |
|  | **Structural timber pine (Treated pine timber)** |  |  |  |  |
| 5 | Timber pine 250x25mm in 6m long to be dressed | 24 | length |  |  |
| 6 | Timber pine 200x50mm in 6m long to be dressed | 30 | length |  |  |
| 7 | Timber pine 150x25mm in 6m long to be dressed | 40 | length |  |  |
| 8 | Timber pine 100x50mm in 6m long to be dressed | 68 | length |  |  |
| 9 | Timber pine 75x50mm in 6m long to be dressed | 62 | length |  |  |
| 10 | Timber pine 50x50mm in 6m long | 36 | length |  |  |
|  | **Roofing Materials** |  |  |  |  |
| 11 | 0.55mm BMT colorbond 15feet 4.58m ` | 64 | sheet |  |  |
| 12 | 0.55mm BMT colorbond 12feet 3.67m | 64 | sheet |  |  |
| 13 | Roof flashing 2.4m | 23 | pcs |  |  |
| 14 | 0.55mm BMT colorbond eaves guttering with bracket | 6 | no |  |  |
| 15 | stop ends | 4 | no |  |  |
| 16 | outlet to gutter | 4 | length |  |  |
| 17 | 100mm diameter upvc downpipe including clips in 6m long | 14 | no |  |  |
| 18 | clip for downpipe | 8 | no |  |  |
| 19 | hydroseal | 7 | tube |  |  |
| 20 | silicone | 7 | pkt |  |  |
| 21 | Rivert (100no/pkt) | 2 | no |  |  |
| 22 | silicone gun | 2 | no |  |  |
| 23 | Rivert gun | 1 | no |  |  |
|  | **Joinery** |  |  |  |  |
| 24 | 100x75mm butt brass hinges with screws | 4 | no |  |  |
| 25 | Rebated mortice lock complete with handles and keys | 2 | no |  |  |
| 26 | 10 blade louver frame | 32 | no |  |  |
| 27 | 36"x 6" (914x150mm) clear glass blade | 320 | no |  |  |
| 28 | polished edges | 6 | no |  |  |
| 29 | solvent cement glue for pvc 500g/tin | 3 | no |  |  |
|  | **Tiling** |  |  |  |  |
| 30 | 300x300mm non-slip ceramic floor tile | 153 | box |  |  |
| 31 | CTF adhesive for ceramic tiles | 76 | pkt |  |  |
| 32 | Tile spacer 2mm | 4 | pkt |  |  |
| 33 | Grout | 4 | bags |  |  |
|  | **Painting and Decorating** |  |  |  |  |
| 34 | Acrylic primer sealer undercoat | 11 | tin |  |  |
| 35 | H/gloss 4ltrs | 15 | tin |  |  |
| 36 | Tray complete with roller and sleeve | 6 | no |  |  |
| 37 | 4 inch paint brush | 6 | no |  |  |
| 38 | 3 inch paint brush | 6 | no |  |  |
|  | **Nails, Screw Bolt** |  |  |  |  |
| 40 | 4" galvanized FC nails 100pcs/pkt | 22 | pkt |  |  |
| 41 | 3" galvanized @ 100pcs/pkt | 15 | pkt |  |  |
| 42 | Flat head nail 2" | 17 | pkt |  |  |
| 43 | 2"x3.15mm bullet head galv nail | 17 | pkt |  |  |
| 44 | 2"x3.15mm clout galv nail | 15 | pkt |  |  |
| 45 | Roofing nails 2" | 7 | no |  |  |
| 46 | 4" counter sunk wood screws | 210 | no |  |  |
| 47 | Dyna bolt | 105 | pcs |  |  |
| 48 | Bolt and nut 9" | 105 | pcs |  |  |
| 49 | Bolt and nut 12" | 15 | pkt |  |  |
| 50 | 3" counter sunk wood screws | 7 | pkt |  |  |
|  | **Total cost** |  |  |  |  |
|  | **vat** |  |  |  |  |
|  |  |  |  |  |  |
|  | **other charges** |  |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |  |