**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **15-G023-23**

## Specification

### Background

The women Centre was a 2009 priority project for the Island Council of Aranuka. It is still an outstanding project for the Island, that is the implementation has been delayed for almost 8 years despite the availability of the project’s fund and which was partly caused as a result of the Island Council changing of decisions regarding the design of the project. However the core purpose for this project is to provide women with a building to bring together of their skills cohesively for the betterment of the Island.

### Requirements

All supporting documentation must be in English. All suppliers are required to submit the following documents.

1. Quotation from the Bidder must be vat inclusive. Note supplier is accountable to pay for the custom duty and delivery charges (Technical components with financial – showing costings).
2. Bank statement (It will determine the supplier capacity)
3. Business License from either BTC & TUC.
4. Time Schedule for supplying of the project materials
5. Tax clearance letter

Please note that the list provided in the Instructions on How to Submit a Quotation template (page 5) are the requirements needed for tender opening. The list above all compiled in the Technical Component (list letter d).

### Installation services

Not Applicable

### Delivery Time

Suppliers are required to provide the delivery timeframe.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Quantity | Price (to be Tendered) |
|  | **Toolls & Sundries** |  |  |  |
|  | Shovels | No. | 4 |  |
|  | Wheel barrow | No. | 2 |  |
|  | Bolt cutter | No. | 1 |  |
|  | Crow bar | No. | 1 |  |
|  | Trowel 200mm pointed | No. | 2 |  |
|  | Trowel blaster | No. | 2 |  |
|  | Circular saw | No. | 1 |  |
|  | Cordless drill | No. | 1 |  |
|  | Lead wire 20m | No. | 1 |  |
|  | Angle grinder | No. | 1 |  |
|  | Block moulds 200mm thick | No. | 1 |  |
|  | Hose 12 mm dimeter 25m | No. | 1 |  |
|  |  |  |  |  |
|  | **Concrete Works (cement type GP or GB) and to be 20MPA Concrete strength** |  |  |  |
|  | 40 kg cement for slab, lintel, beam, block grout and screeding | bags | 144 |  |
|  | 40 kg cemen (1240 concrete blocks 200mm thick) | bags | 67 |  |
|  | Aggregates | M3 |  |  |
|  | Sand | M3 |  |  |
|  | Polythene | roll | 2 |  |
|  | Tie wire | No. | 5 |  |
|  |  |  |  |  |
|  | **Formwork** |  |  |  |
|  | Formply 1 inch | sht | 11 |  |
|  | Timber pine 50x50mm | Length | 13 |  |
|  |  |  |  |  |
|  | **Reinforcement** |  |  |  |
|  | Arc Fabric mesh wire 5.5m x2.13m (59m2) | Length | 6 |  |
|  | Rod 16mm dia. Reinforcing bar in 6m length (6m) | Length | 1 |  |
|  | Rod 10mm dia. Reinforcing bar 6m length (434m) | Length | 80 |  |
|  | Rod 12mm dia. Reinforcing bar in 6m length (167m) | Length | 31 |  |
|  | Rod 6 dia. Reinforcing bar in 6m length (284) | Length | 52 |  |
|  | **Metal Work** |  |  |  |
|  | 100x100mm square tube metal for door and window jamb & header | Length | 8 |  |
|  | **Timber works** |  |  |  |
|  | 200 x25mm fascia board | Length | 9 |  |
|  | 100 x50mm timber pine | length | 65 |  |
|  | 50 x25mm timber pine moulded skirting | length | 7 |  |
|  | 50 x25mm bird batten | length | 42 |  |
|  | 20 x20mm timber pine | Length | 13 |  |
|  | Timber louver to gable 6 x2 | Length | 3 |  |
|  |  |  |  |  |
|  | **Dressed Timber** |  |  |  |
|  | 200 x 50mm dressed for header, mullion and sill | length | 7 |  |
|  | 100 x50mm dressed dakua for door and window head and jamb | Length | 9 |  |
|  |  |  |  |  |
|  | **Tiles** |  |  |  |
|  | **Floor** |  |  |  |
|  | 150 x150mm ceramic floor tile (2m2/box) | Box | 6 |  |
|  | Vinyle tile 300 x300mm (4.5m2/box) | Box | 3 |  |
|  | Adhesive for vinyle tile 4 litres | Tin | 3 |  |
|  | Ceremic wall tile 150 x50 (2m2/box) | Box | 7 |  |
|  | Adhesive for ceremic tile 20 kilo | Bag | 6 |  |
|  | Allow for tile spacer | Item | 1 |  |
|  |  |  |  |  |
|  | **Ceiling** |  |  |  |
|  | Plywood lining on ceiling noggings (4.5mm thick) | Shts | 18 |  |
|  | Plywood lining soffit cladding (4.5mm thick) | Shts | 3 |  |
|  | 12mm plywood for gusset | Shts | 5 |  |
|  | Fabric mesh wire ceiling to cells | Shts | 2 |  |
|  |  |  |  |  |
|  | **Roof Plumbing** |  |  |  |
|  | Corrugated Zincalum Roof Decking |  |  |  |
|  | 8ft zincalum rooing | Shts | 76 |  |
|  | Alum. Foil sisalation @1.2 x60m in length | Roll | 2 |  |
|  | Alum ridge capping @2.4m/pcs | Pcs | 5 |  |
|  | Alum barge flashing @2.4m/pcs | Pcs | 8 |  |
|  | Alum fascia gutter @2.4m/pcs | Pcs | 21 |  |
|  | Stop ends joint to gutter | No. | 4 |  |
|  | 100mm di vent cowl | No. | 1 |  |
|  | 100mm diameter pvc downpipe and vent | Length | 3 |  |
|  | 100mm diameter bend | No. | 4 |  |
|  | Gutter Outlet 100 dia | No. | 2 |  |
|  | Rivert gun | No. | 1 |  |
|  | Blind rivert 4.6mm @ 100no/pkt | Pkt | 1 |  |
|  | Silicone | Tube | 1 |  |
|  | Silicone gun | No. | 1 |  |
|  | **Doors and windows** |  |  |  |
|  | Internal panel door 40 x 800 x2100mm | No. | 2 |  |
|  | External panel door 40 x850 x2100mm hung in pairs | No. | 1 |  |
|  | External panel door 40 x350 x21000mm hung in pairs | No. | 1 |  |
|  | Cell door 100 x920 x2060mm complete with lock and hinges | No. | 3 |  |
|  | 10 blade louvre frame black | Prs | 10 |  |
|  | 914 x150mm clear glass blade | No. | 100 |  |
|  | 100mm butt brass hinges | Prs | 8 |  |
|  | Rebated mortice lock with handles | Set | 3 |  |
|  | Mortice lock with handles | Set | 1 |  |
|  | 150mm barrel bolt complete with screw | No. | 2 |  |
|  | **Plumbing** |  |  |  |
|  | Pvc pipe 15mm distribution line (overhead) | Length | 3 |  |
|  | Elbow pvc 15mm | No. | 4 |  |
|  | 15mm dia. Pvc tee | No. | 2 |  |
|  | Male adapator 15mm | No. | 5 |  |
|  | Female adapator 15mm | No. | 2 |  |
|  | Gate valve brass ½’’ | No. | 2 |  |
|  | Pilla tap 15mm | No. | 1 |  |
|  | Reducing bush25mm x 15mm | No. | 1 |  |
|  | 25mm elbow | No. | 4 |  |
|  | 25mm pvc pipe | Length | 3 |  |
|  | **WC & CELL** |  |  |  |
|  | Elbow 100mm dia, PVC 90 degrees | No. | 3 |  |
|  | Tee connector 100mm dia. Pvc | No. | 1 |  |
|  | Male adaptor 25mm | No. | 7 |  |
|  | Reducing bush 100mm x 32mm 90 degrees | No. | 1 |  |
|  | 32mm dia. Elbow 90degree | No. | 1 |  |
|  | Gully trap 32mm dia, | No. | 2 |  |
|  | 32mm dia. Elbow 45 degree | No. | 1 |  |
|  | Tee connector 32mm dia. Pvc | No. | 1 |  |
|  | Pvc pipe 100mm dia | Length | 2 |  |
|  | Pan white ‘P’ trap | Pcs | 1 |  |
|  | Pan seet | No. | 1 |  |
|  | Vent cap 100mm pvc | No. | 1 |  |
|  | Wash hand basin c/w bracket, and plug and waste | No. | 1 |  |
|  | S-trap 32mm diameter | No. | 1 |  |
|  | 32mm dia. Elbow 90 degree | no | 1 |  |
|  | Pvc pipe 32mm | Length | 2 |  |
|  | **Transimittion Line** |  |  |  |
|  | Elbow pvc 25mm 90 degree | No | 4 |  |
|  | Union socket 25mm | No | 1 |  |
|  | Male adapator 25mm | No. | 1 |  |
|  | Female adapator 25mm | No. | 1 |  |
|  | 25mm pvc pipe | Length | 3 |  |
|  | **Suction Inlet Pumb** |  |  |  |
|  | Elbow pvc 25mm 90 degree | No. | 4 |  |
|  | Union socket 25mm | No. | 2 |  |
|  | Tee connector 25mm dia. Pvc | No. | 1 |  |
|  | Male adapator 25mm | No. | 3 |  |
|  | Foot valve 25mm | No. | 1 |  |
|  | 25mm pvc pipe | Length | 3 |  |
|  | Thread tape | No. | 2 |  |
|  | Solvent cement 500g | No. | 4 |  |
|  | Clip pvc 15mm | No. | 5 |  |
|  | Pvc clips 25mm | No. | 5 |  |
|  | Clip pvc 100mm | No. | 4 |  |
|  |  |  |  |  |
|  | **Electricals** |  |  |  |
|  | 4’0’’ fluorescent light fittings complete | No. | 4 |  |
|  | Pendant light complete with holder | No. | 3 |  |
|  | Light switch one way | No. | 6 |  |
|  | 1.5mm cable | M | 70 |  |
|  | 2.5mm cable | M | 10 |  |
|  | Mounting block | No. | 7 |  |
|  | Junction box | No. | 8 |  |
|  | Earthing cable 6mm | M | 12 |  |
|  | Earthing rod ¾’’ galvanised pipe | No. | 1 |  |
|  | Insulating tape | No. | 6 |  |
|  | Double power point | No. | 1 |  |
|  | 15mm dia pvc pipe for conduiting | Length | 3 |  |
|  | 15mm pvc clip | No. | 24 |  |
|  | Ceiling fan complete with fan switch | No. | 2 |  |
|  | Allow for clips, junctions and screws | Item | 1 |  |
|  | Switch board with neutral bar | No. | 1 |  |
|  | Circuit breaker 20A | No. | 1 |  |
|  | Circuit breaker 16A | No. | 1 |  |
|  | Circuit breaker 10A | No. | 1 |  |
|  | Circuit breaker 8A | No. | 1 |  |
|  | Wall plug | M | 2 |  |
|  |  |  |  |  |
|  | **Painting** |  |  |  |
|  | Pink primer 4 litres | Tins | 7 |  |
|  | Undercoat 4 litres | Tins | 12 |  |
|  | H/gloss 4 litres | Tins | 10 |  |
|  | Acrylic 4 litres | Tins | 12 |  |
|  | Tray complete with roller and sleeve | No. | 3 |  |
|  | 4’’ paint brush | No. | 4 |  |
|  | 3’’ paint brush | No. | 4 |  |
|  | 2’’ paint brush | No. | 5 |  |
|  | 1’’ paint brush | No. | 6 |  |
|  |  |  |  |  |
|  | **Nails, Screws & Bolts** |  |  |  |
|  | 4’’ galvanised nail | Kg | 25 |  |
|  | 3’’ galvanised nail | Kg | 25 |  |
|  | 2 1/2’’ galvanised nail | Kg | 15 |  |
|  | 2’’ galvanised nail flat head | Kg | 15 |  |
|  | 2 ½’’ twisted roof nail | Kg | 20 |  |
|  | 12mm dia. Bolt and nuts | No. | 50 |  |
|  |  |  |  |  |
|  | **Exterior Element** |  |  |  |
|  | **Water Services** |  |  |  |
|  | Water tank 5000 litres | No | 1 |  |
|  | Polythene tank 1200 litres | No. | 1 |  |
|  | Solvent cement 500g | No. | 2 |  |
|  |  |  |  |  |
|  | **Rainwater tanks/ Header tank** |  |  |  |
|  | **Rainwater Concrete Base** |  |  |  |
|  | Cement 40kg | Bags | 17 |  |
|  | Cement for brick manufacture | Bags | 2 |  |
|  | F62 fabric mesh wire 6mx2.4m/sheet | Sht | 1 |  |
|  | Rod 12mm diameter 6m | Length | 3 |  |
|  | Rod 6mm diameter 6m | Length | 2 |  |
|  | Tie wire | No | 1 |  |
|  | Fine aggregate | M3 | 2 |  |
|  | Coarse aggregate | M3 | 2 |  |
|  | 200x25mm timber formwork | Length | 2 |  |
|  | 100x50mm formwork frames | Length | 2 |  |
|  |  |  |  |  |
|  | **Overhead tank Stand** |  |  |  |
|  | Cement 40 kg | Bags | 28 |  |
|  | Cement for brick manufacture | Bags | 6 |  |
|  | F62 fabric mesh wire 6mx2.4m/sheet | Sht | 1 |  |
|  | Rod 12mm diameter 6m | Length | 6 |  |
|  | fine aggregate | M3 | 2 |  |
|  | Coarse aggregate | M3 | 4 |  |
|  | 200x25mm timber formwork | Length | 2 |  |
|  | Formwork plasply boarding | Sht | 12 |  |
|  | 100x50mm formwork frames | Length | 4 |  |
|  | Davey water pumb | No | 1 |  |
|  | Concrete for precast concrete well ring size: 1200mm dia x 700mm high | Bags | 6 |  |
|  |  |  |  |  |
|  | **Septic Tank and Soakaway Pit** |  |  |  |
|  | **Septic Tank** |  |  |  |
|  | Cement 40kg | Bags | 40 |  |
|  | Cement for brick manufacture | Bags | 15 |  |
|  | F62 fabric mesh wire 6m2.4m/sheet | Sht | 3 |  |
|  | Rod 16mm diameter 6m | Length | 11 |  |
|  | Rod 12mm diameter 6m | Length | 10 |  |
|  | Rod 6mm diameter 6m | Length | 2 |  |
|  | Fine aggregate | M3 | 2 |  |
|  | Coarse aggregate | M3 | 4 |  |
|  | 200x25mm timber formwork | Length | 2 |  |
|  | Formwork plasply boarding | Sht | 8 |  |
|  | 100x50mm formwork frames | Length | 4 |  |
|  |  |  |  |  |
|  | **Soakaway Pit** |  |  |  |
|  | Cement 40kg | Bags | 16 |  |
|  | Cement for brick manufacture | Bags | 5 |  |
|  | F62 fabric mesh wire 6mx2.4m/sheet | Sht | 1 |  |
|  | Fine aggregate | M3 | 2 |  |
|  | Coarse aggregate | M3 | 4 |  |
|  | **Drainage** |  |  |  |
|  | 40mm dia pvc pipe 6m in length for drainage | Length | 5 |  |
|  | 40mm diameter pvc pipe bend | No. | 5 |  |
|  | 40mm diameter pvc tee | No. | 2 |  |
|  | 100mm dia pvc pipe 6m in length for drainage | Length | 3 |  |
|  | 100mm dia pvc bend | No. | 2 |  |
|  | 100mm dia pvc tee with inspection cap | No. | 1 |  |
|  | 100mm dia pvc tee | No. | 4 |  |
|  | **Furniture** |  |  |  |
|  | Counter with Seat | Item | 1 |  |