**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **15-G037-23**

## Specification

### Background

Te Bouateaina Maneaba was a 2023 priority project for Butaritari island council. It is still an outstanding project for the island, that is the implementation has been delayed despite the availability of the disaster fund. The council has been looking for an adequate design to avoid future destructions from natural disasters. The core purpose of the maneaba is to accommodate Butaritari people that are visiting Tarawa, for economic development through rentals of the maneaba and functions of the island that were to be held in Tarawa.

### Requirements

All supporting documentation must be in English.

1. Quotation from the Bidder must be vat inclusive. Note supplier is accountable to pay for the custom duty and delivery charges (Technical components with financial – showing costings).
2. Business Registration from MCIC ***for local suppliers only***
3. Business License from either BTC & TUC ***for local suppliers only***
4. Time Schedule for supplying of the project materials

Please note the list of required documents for tender opening are stated in the ***Instructions on How to Submit a Quotation*** template, page 5.

### Installation services

Not applicable

### Delivery Time

Suppliers are required to provide the delivery timeframe.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Unit | Quantity | Price (to be Tendered) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 1 | **Timber Roofing** | **Australian Pine**, 250\*50mm、250\*100mm、300\*100mm、150\*50mm、75\*50mm，1 layer **OIL BASED PRIMER SEALER UNDERCOAT**, 2 layers of **SEMI-GLOSS ENAMEL** ，thickness **200μm** | m3 | 23.76 |  |
| 2 | **Bracket and other steel part** | Q355B,S355JR,SM490,ASTM A572 50ksi,  clean steel to Sa2.5 Grade,  **Hot-dipped galvanized, Zinc 600g/m2** | ton | 0.66 |  |
| **B** | **Roof System** | | | |  | |
| 1 | **Roof panel** | 0.5mm **Zincalume** Sheeting，**Baogang** brand  **sea blue** color (RAL5015) | m | 1235.60 |  |
| 2 | window | painted timber louver | m2 | 63.88 |  |
| 3 | outside guardrail | made by stainless steel pipe | m | 7.80 |  |
| 4 | Trim & Flashing | made by 0.5mm steel sheet | m | 297 |  |
| 5 | fittings | self-tapping crew, glass cement etc. | m2 | 1037.91 |  |
| **C** | **Fittings** | | | |  | |
| 1 | **Embedded bolts** | M16 foundation bolt ，Galvanized | pcs | 48 |  |
| 2 | embedded bar | M12 rebar, Galvanized | set | 144 |  |
| 3 | expansion bolt | M12，Galvanized | set | 48 |  |
| 4 | Gutter | **0.8mm** **Zincalume** sheet | m | 97 |  |
| 5 | downspout | 100\*80 Aluminu pipe | m | 66 |  |