**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **43-G003-23**

## Specification

### Background

The idea of reviving the old Fire pump is one of the company's priorities as outlined in its business plan and budget. The replacement of the entire old fire-pump is critical to ensuring long-term business sustainability and profitability. As part of the Occupational Health and Safety regulations in an industrial environment, a fire exhauster unit is a vital feature of the business operation that makes the workplace safe for employees and prevents unforeseen fire occurrences inside the company's operation.

Long-term fire prevention is required in any industrial operation. The existing fire pump is currently experiencing repeated malfunctions, while the parts are obsolete in the market and unsafe for the company's overall operation as well as for employees. It is vital to get a new fire-pump with updated features and automated maneuvers that are considerably more effective in reducing fire dangers and emergency accidents. The required and chosen specifications of the required fire-pump are one-of-a-kind in accordance with the company's requirements and standards.

### Requirements

The following requirements must be met:

|  |  |
| --- | --- |
| **General requirement** | |
| Inlet Diameter | 100mm |
| Outlet Diameter | 80mm |
| Power Source | Diesel fuel & Electrical Supply |
| Unit Pumps | Electric Pump |
|  | Diesel Pump |
|  | Jockey Pump |
| Speed | 2900 rpm |
| Pressure | 195 psi |
| Diesel Pump accessories | Radiator, Silencer, Fuel tank |
| Other package requirement | Control Panel - |
|  | Other accessories are to check |
| Manufacturer is recommended |  |

### Tenderer’s required documentation

All supporting documentation must be in English. The following supporting documents should be provided.

1. Business Registration with nature of business indication that the tenderer is capable to order Flexi tanks in bulk. Failure to provide such registration will result in disqualification of the tenderer. This is applicable only for international Tenderers.
2. Signed certificate for compliance form should be provided. (Failure will result in disqualifying the tenderer)
3. Valid business license from the relevant Councils
4. Tax clearance letter from Tax Office for tax registered companies (Failure to provide will result in rejection of the tender)
5. Bank statement (To ensure the companies have their financial capacity to do the procurement, this requirement should be provided. Failure to provide will result in the disqualification of the tender)
6. A complete quotation for financial component of the proposal
7. A complete technical requirement in achieving the specifications of goods indicated in this “Specification template”.

### Installation services

Not applicable

### Delivery Time

Not applicable

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | Fire-pump 195psi | 1 |  |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |