**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **15-G005-24**

## Specification

### Background

The living quarter was one of Nonouti priority project in 2009. It is still an outstanding project for the Island, that is the implementation for the rest of the living quarter has completed however, the council request for the remaining fund to be utilized to construct the Clerk’s house. The clerk’s house was first initiated in 2022 which is now in the stage of procurement. The core purpose for this project is to provide a comfortable and safe shelter for the Clerk.

### Requirements

All supporting documentation must be in English. All suppliers are required to submit the following documents.

1. Quotation from the Bidder must be vat inclusive. Note supplier is accountable to pay for the custom duty and delivery charges (Technical components with financial – showing costings).
2. Business Registration from MCIC – must be recently certified
3. Business License from either BTC & TUC.
4. Time Schedule for supplying of the project materials
5. Tax clearance letter from Tax office (MFED Bairiki)

### Installation services

Not applicable

### Delivery Time

Suppliers are required to provide the delivery timeframe. Should be within 60 days.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Quantity | Price (to be Tendered) |
|  | **Concrete work** |  |  |  |
|  | Strip Footing | Bag | 24 |  |
|  | Floor slap | Bag | 55 |  |
|  | Brick Laying cement | Bag | 30 |  |
|  | Bricks | Block | 1036 |  |
|  | **Formwork** |  |  |  |
|  | Fascia Board 8 × 1 | Length | 13 |  |
|  | **Ceiling work** |  |  |  |
|  | Plywood construction (3/16’’) | Sheet | 45 |  |
|  | 2×2 timber for ceiling nogging | Length | 38 |  |
|  | **Reinforcement** |  |  |  |
|  | D16 rod | Length | 24 |  |
|  | Mesh wire | Sheet | 3 |  |
|  | Polythene | Roll | 1 |  |
|  | Tie wire | Roll | 3 |  |
|  | D12 rod (Stirrups) | Length | 26 |  |
|  | **Timber work** |  |  |  |
|  | 4×2 window | Length | 25 |  |
|  | 4×2 rafter | Length | 36 |  |
|  | 3×2 purlin | Length | 24 |  |
|  | Door flame (6×2) | Length | 4 |  |
|  | 2×2 – door (studs) | Length | 9 |  |
|  | Interior Partition (3×2) | Length | 28 |  |
|  | 6×1 – Fascia | Length | 9 |  |
|  | 6×2 – top plate | Length | 16 |  |
|  | **Window work** |  |  |  |
|  | Louver frame (10 louvers) | Pair | 24 |  |
|  | Louver frame (4 louvers) | Pair | 1 |  |
|  | Louver glass | Length | 246 |  |
|  | **Door work** |  |  |  |
|  | Hinges | Pair | 7 |  |
|  | Entrance lock | Unit | 6 |  |
|  | **Roof work** |  |  |  |
|  | Roofing sheet 9ft | Sheet | 42 |  |
|  | Roofing sheet 6ft | Sheet | 42 |  |
|  | Ridge cap | Length | 6 |  |
|  | **Electrical work** |  |  |  |
|  | Fluorescent light (4fts) | Set | 10 |  |
|  | Switch light (double) | Set | 5 |  |
|  | Power point (double) | Set | 5 |  |
|  | Power point (single) | Set | 5 |  |
|  | Wire @2.5mm | Roll | 2 |  |
|  | Wire clip | Set | 2 |  |
|  | **Plumbing work** |  |  |  |
|  | Bowl | Set | 1 |  |
|  | Floor grade | Unit | 1 |  |
|  | Sink | Set | 1 |  |
|  | Pipe (50mm) | Length | 1 |  |
|  | Elbow (50mm) | Unit | 2 |  |
|  | Elbow (100mm) | Unit | 2 |  |
|  | Reducer 100mm – 50mm | Unit | 1 |  |
|  | Gutter | Length | 12 |  |
|  | Bracket | Unit | 44 |  |
|  |  |  |  |  |
|  | Hardware |  |  |  |
|  | Roofing nail | Kg | 10 |  |
|  | 2’’ nail | Kg | 5 |  |
|  | 3’’ nail | Kg | 5 |  |
|  | 4’’ nail | Kg | 15 |  |
|  | Ceramic tile | Box | 64 |  |
|  | ATF – tile glue / cement | Bag | 32 |  |
|  | Bolt 6’’ | No. | 30 |  |
|  | Undercoat paint | Tin | 4 |  |
|  | Pink primer | Tin | 3 |  |
|  | Roll brush | Set | 3 |  |
|  | Paint brush 4’’ | No. | 5 |  |
|  |  |  |  |  |