**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **15-G040-23**

## Specification

### Background

The project was proposed by Beru Island Council to accommodate the need of the People on Beru Island to build a Police Office and Cell to give a better place for the island people. The project is new, and will commence once every part of the process is completed.

### Requirements

All supporting documentation must be in English. Kindly note that the list of requirement can be found in the **Instructions on How to Submit Tender** template, page 5.

### Delivery Time

Suppliers are required to provide the delivery time frame.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pos. | Description | Unit | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
|  | *Tools & Sundries* |  |  |  |  |
| 1 | Shovels | no. | 4 |  |  |
| 2 | Wheel Barrows | no. | 2 |  |  |
| 3 | Bolt Cutter | no. | 1 |  |  |
| 4 | Crow Bars | no. | 1 |  |  |
| 5 | Trowel 200mm pointed | no. | 2 |  |  |
| 6 | Trowel plaster | no. | 2 |  |  |
| 7 | Circular Saw | no. | 1 |  |  |
| 8 | Block mould 200mm thick | no. | 1 |  |  |
| 9 | Cordless drill | no. | 1 |  |  |
| 10 | Leadwire 20m | no. | 1 |  |  |
| 11 | Angle grinder | no. | 1 |  |  |
| 12 | Hose 12mm diameter 25m | no. | 1 |  |  |
|  | *Concrete Works* |  |  |  |  |
| 13 | 40kg cement for slab, lintel, beam, block grout and seceding | bags | 144 |  |  |
| 14 | 40kg cement (1240 concrete blocks 200mm thick) | bags | 67 |  |  |
| 15 | Polythene | m3 | 2 |  |  |
| 16 | Tie wire | m3 | 5 |  |  |
|  | *Formwork* |  |  |  |  |
| 17 | Formply 1 inch | roll | 11 |  |  |
| 18 | Timber Pine 50x50mm | no. | 13 |  |  |
|  | *Reinforcement* |  |  |  |  |
| 19 | Arc Fabric mesh wire 5.5mx2, 13m (59m2) | sht | 6 |  |  |
| 20 | Rod 16mm dia. Reinforcing bar in 6m length (6m) | leng | 1 |  |  |
| 21 | Rod 10mm dia. Reinforcing bar in 6m length (434m) | sht | 80 |  |  |
| 22 | Rod 12mm dia. Reinforcing bar in 6m length (167m) | leng | 31 |  |  |
| 23 | Rod 6mm dia. Reinforcing bar in 6m length (284m) | leng | 52 |  |  |
|  | *Metal Work* |  |  |  |  |
| 24 | 100mm x 100mm square tube metal for door and window jamb and header | leng | 8 |  |  |
|  | *Timber Works* |  |  |  |  |
| 25 | 200x25mm fascia board | leng | 9 |  |  |
| 26 | 100x50mm timber pine | leng | 65 |  |  |
| 27 | 50x25mm timber pine moulded skirting | leng | 7 |  |  |
| 28 | 50x25mm bird batten | leng | 42 |  |  |
| 29 | 20x20mm timber pine | leng | 13 |  |  |
| 30 | Timber louver to gable 6x2 | leng | 3 |  |  |
|  | *Dressed Timber* |  |  |  |  |
| 31 | 200x50mm dressed dakua for header, mullion and sill | leng | 7 |  |  |
| 32 | 100x50mm dressed dakua for door and window head and jamb | leng | 9 |  |  |
|  | *Tiles*  Floor |  |  |  |  |
| 34 | 150x150mm ceramic floor tile (2m2/box) | box | 6 |  |  |
| 35 | Vinyle tile 300x300mm (4.5m2/box) | box | 3 |  |  |
| 36 | Adhesive for vinyle tile 4liters | Tin | 3 |  |  |
| 37 | Ceramic Wall tile 150x150 (2m2/box) | box | 7 |  |  |
| 38 | Adhesive for ceramic tile 20kilo | bag | 6 |  |  |
| 39 | Allow for tile spacer | pkt | 1 |  |  |
|  | *Ceiling* |  |  |  |  |
| 40 | Plywood lining on ceiling noggins (4.5mm thick) | sht | 18 |  |  |
| 41 | Plywood lining for soffit cladding (4.5mm thick) | sht | 3 |  |  |
| 42 | 12mm plywood for gusset | sht | 5 |  |  |
| 43 | Fabric Mesh Wire ceiling to cells | sht | 2 |  |  |
|  | *Roofing Plumbing* |  |  |  |  |
| 44 | Corrugated zincalcum road decking |  |  |  |  |
| 45 | 8ft zincalum roofing | sht | 76 |  |  |
| 46 | Alum Foil sisalation @ 1.2x60m in length | roll | 2 |  |  |
| 47 | Alum ridge capping @ 2.4m/pcs | pcs | 5 |  |  |
| 48 | Alum barge flashing @ 2.4m/pcs | pcs | 8 |  |  |
| 49 | Alum fascia gutter @ 2.4m/pcs | pcs | 21 |  |  |
| 50 | Stop ends joint to gutter | no. | 4 |  |  |
| 51 | 100mm dia. vent cowl | no. | 1 |  |  |
| 52 | 100mm dia. pvc downpipe and vent | leng | 3 |  |  |
| 53 | 100mm diameter bend | no. | 4 |  |  |
| 54 | Gutter outlet 100mm dia. | no. | 2 |  |  |
| 55 | Rivert gun | no. | 1 |  |  |
| 56 | Blind rivert 4.6mm @ 100no/pkt | pkt | 1 |  |  |
| 57 | Silicone | tube | 1 |  |  |
| 58 | Silicone gun | no. | 1 |  |  |
|  | *Doors and Windows* |  |  |  |  |
| 59 | Internal panel door 40x800x2100mm | no. | 2 |  |  |
| 60 | External panel door 40x850x2100mm hung in pairs | no. | 1 |  |  |
| 61 | External panel door 40x350x2100mm hung in pairs | no. | 1 |  |  |
| 62 | Cell door 100x920x2060mm complete with lock and hinges | no. | 3 |  |  |
| 63 | 10 blade louver frame black | prs | 10 |  |  |
| 64 | 914x150mm clear glass blade | no. | 100 |  |  |
| 65 | 100mm butt brass hinges | prs | 8 |  |  |
| 66 | Rebated mortice lock with handles | set | 3 |  |  |
| 67 | Mortice lock with handles | set | 1 |  |  |
| 68 | 150mm barrel bolt complete with screw | no. | 2 |  |  |
|  | *Plumbing* |  |  |  |  |
| 69 | Pvc pipe 15mm distribution line (overhead) | leng | 3 |  |  |
| 70 | Elbow pvc 15mm | no. | 4 |  |  |
| 71 | 15mm dia. Pvc tee | no. | 2 |  |  |
| 72 | Male adaptor 15mm | no. | 5 |  |  |
| 73 | Female adaptor 15mm | no. | 2 |  |  |
| 74 | Gate valve brass ½” | no. | 2 |  |  |
| 75 | Pilla tap 15mm | no. | 1 |  |  |
| 76 | Reducing bush 25mm x 15mm | no. | 1 |  |  |
| 77 | 25mm elbow | no. | 4 |  |  |
| 78 | 25mm pvc pipe | leng | 3 |  |  |
|  | WC & Cell |  |  |  |  |
| 79 | Elbow 100mm dia. Pvc 90degree | no. | 3 |  |  |
| 80 | Tee connector 100mm dia. Pvc | no. | 1 |  |  |
| 81 | Male adaptor 25mm | no. | 7 |  |  |
| 82 | Reducing bush 100mm x 32mm 90degree | no. | 1 |  |  |
| 83 | 32mm dia. Elbow 90 degree | no. | 1 |  |  |
| 84 | Gully trap 32mm dia. | no. | 2 |  |  |
| 85 | 32mm dia. Elbow 45 degree | no. | 1 |  |  |
| 86 | Tee connector 32mm dia. Pvc | no. | 1 |  |  |
| 87 | Pvc pipe 100mm dia. | leng | 2 |  |  |
| 88 | Pan white “P” trap | pcs | 1 |  |  |
| 89 | Pan seat | no. | 1 |  |  |
| 90 | Vent cap 100mm pvc | no. | 1 |  |  |
| 91 | Wash hand basin c/w bracket, and plug and waste | no. | 1 |  |  |
| 92 | S-trap 32mm diameter | no. | 1 |  |  |
| 93 | 32mm dia. Elbow 90degree | no. | 1 |  |  |
| 94 | Pvc pipe 32mm | leng | 2 |  |  |
|  | Transmission Line |  |  |  |  |
| 95 | Elbow pvc 25mm 90degree | no. | 4 |  |  |
| 96 | Union socket 25mm | no. | 1 |  |  |
| 97 | Male adaptor 25mm | no. | 1 |  |  |
| 98 | Female adaptor 25mm | no. | 1 |  |  |
| 99 | 25mm pvc pipe | leng | 3 |  |  |
|  | Suction Inlet Pump |  |  |  |  |
| 100 | Elbow pvc 25mm 90degree | no. | 4 |  |  |
| 101 | Union socket 25mm | no. | 2 |  |  |
| 102 | Tee connector 25mm dia. Pvc | no. | 1 |  |  |
| 103 | Male adaptor 25mm | no. | 3 |  |  |
| 104 | Foot valve 25mm | no. | 1 |  |  |
| 105 | 25mm pvc pipe | leng | 3 |  |  |
| 106 | Thread tape | no. | 2 |  |  |
| 107 | Solvent cement 500g | no. | 4 |  |  |
| 108 | Clip pvc 15mm | no. | 5 |  |  |
| 109 | Pvc clips 25mm | no. | 5 |  |  |
| 110 | Clip pvc 100mm | no. | 4 |  |  |
|  | *Electricals* |  |  |  |  |
| 111 | 4’0” fluorescent light fittings complete | no. | 4 |  |  |
| 112 | Pendant light complete with holder | no. | 3 |  |  |
| 113 | Light switch one way | no. | 6 |  |  |
| 114 | 1.5mm cable | m | 70 |  |  |
| 115 | 2.5mm cable | m | 10 |  |  |
| 116 | Mounting Block | no. | 7 |  |  |
| 117 | Junction box | no. | 8 |  |  |
| 118 | Earthing cable 6mm | m | 12 |  |  |
| 119 | Earthing rod ¾” galvanized pipe | no. | 1 |  |  |
| 120 | Insulating tape | no. | 6 |  |  |
| 121 | Double power point | no. | 1 |  |  |
| 122 | 15mm dia. Pvc pipe for conducting | leng | 3 |  |  |
| 123 | 15mm pvc clip | no. | 24 |  |  |
| 124 | Ceiling fan complete with fan switch | no. | 2 |  |  |
| 125 | Allow for clips, junctions and screws | item | 1 |  |  |
| 126 | Switch board with neutral bar | no. | 1 |  |  |
| 127 | Circuit breaker 20A | no. | 1 |  |  |
| 128 | Circuit breaker 16A | no. | 1 |  |  |
| 129 | Circuit breaker 10A | no. | 1 |  |  |
| 130 | Circuit breaker 8A | no. | 1 |  |  |
| 131 | Wall plug | m | 2 |  |  |
|  | *Painting* |  |  |  |  |
| 132 | Pink primer 4L | tin | 7 |  |  |
| 133 | Undercoat 4L | tin | 12 |  |  |
| 134 | H/gloss 4L | tin | 10 |  |  |
| 135 | Acrylic 4L | tin | 12 |  |  |
| 136 | Tray complete with roller and sleeve | no. | 3 |  |  |
| 137 | 4” paint brush | no. | 4 |  |  |
| 138 | 3” paint brush | no. | 4 |  |  |
| 139 | 2” paint brush | no. | 5 |  |  |
| 140 | 1” paint brush | no. | 6 |  |  |
|  | *Nails, Screws & Bolts* |  |  |  |  |
| 141 | 4” galvanized nail | kg | 25 |  |  |
| 142 | 3” galvanized nail | kg | 25 |  |  |
| 143 | 2 ½ ” galvanized nail | kg | 15 |  |  |
| 144 | 2” galvanized nail flat head | kg | 15 |  |  |
| 145 | 2 ½” twisted roof nail | kg | 20 |  |  |
| 146 | 12mm dia. Bolts & nuts | no. | 50 |  |  |
|  | *Exterior Element* |  |  |  |  |
|  | Water Services |  |  |  |  |
| 147 | Water tank 5000 liters | no. | 1 |  |  |
| 148 | Polythene tank 1200 ltrs | no. | 1 |  |  |
| 149 | Solvent cement 500kg | no. | 2 |  |  |
|  | *Rainwater Tanks / Header Tank* |  |  |  |  |
|  | Rainwater Concrete Base: |  |  |  |  |
| 150 | Cement 40kg | bag | 17 |  |  |
| 151 | Cement for brick manufacture | bag | 2 |  |  |
| 152 | F62 fabric mesh wire 6mx2.4m/sheet | sht | 1 |  |  |
| 153 | Rod 12mm dia. 6m | leng | 3 |  |  |
| 154 | Rod 6mm dia. 6m | leng | 2 |  |  |
| 155 | Tie wire | no. | 1 |  |  |
| 156 | 200x25mm timber formwork | leng | 2 |  |  |
| 157 | 100x50mm formwork frames | leng | 2 |  |  |
|  | Overhead Tank Stand: |  |  |  |  |
| 158 | Cement 40kg | bag | 28 |  |  |
| 159 | Cement for brick manufacture | bag | 6 |  |  |
| 160 | F62 fabric mesh wire 6mx2.4m/sheet | bag | 1 |  |  |
| 161 | Rod 12mm dia. 6m | leng | 6 |  |  |
| 162 | 200x25mm timber formwork | leng | 2 |  |  |
| 163 | Formwork plasply boarding | sht | 12 |  |  |
| 164 | 100x50mm formwork frames | leng | 4 |  |  |
| 165 | Davey water pump | no. | 1 |  |  |
| 166 | Concrete for precast concrete well ring size: 1200mm dia. X 700mm high | bag | 6 |  |  |
|  | *Septic Tank and Soakaway Pit* |  |  |  |  |
|  | Septic Tanks: |  |  |  |  |
| 167 | Cement 40kg | bag | 40 |  |  |
| 168 | Cement for brick manufacture | bag | 15 |  |  |
| 169 | F62 fabrick mesh wire 6mx2.4m/sheet | sht | 3 |  |  |
| 170 | Rod 16mm dia. 6m | leng | 11 |  |  |
| 171 | Rod 12mm diameter 6m | leng | 10 |  |  |
| 172 | Rod 6mm dia. 6m | leng | 2 |  |  |
| 173 | 200x25mm Timber formwork | leng | 2 |  |  |
| 174 | Formwork plasply boarding | sht | 8 |  |  |
| 175 | 100x50mm formwork frames | leng | 4 |  |  |
|  | *Soakaway Pit* |  |  |  |  |
| 176 | Cement 40kg | bag | 16 |  |  |
| 177 | Cement for brick manufacture | bag | 5 |  |  |
| 178 | F62 fabric mesh wire 6mx2.4m/sheet | sht | 1 |  |  |
|  | *Drainage* |  |  |  |  |
| 179 | 40mm dia. Pvc pipe 6m in length for drainage | leng | 5 |  |  |
| 180 | 40mm dia. Pvc pipe bend | no. | 5 |  |  |
| 181 | 40mm dia. Pvc tee | no. | 2 |  |  |
| 182 | 100mm dia. Pvc pipe 6m in length for drainage | leng | 3 |  |  |
| 183 | 100mm dia. Pvc bend | no. | 2 |  |  |
| 184 | 100mm dia. Pvc tee with inpection cap | no. | 1 |  |  |
| 185 | 100mm dia. Pvc tee | no. | 4 |  |  |
|  | *Furniture* |  |  |  |  |
| 186 | Counter with Seat | item | 1 |  |  |