**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **RFQ-15-G015-24**

## Specification

### Background

The project was proposed by Beru Island Council to accommodate the need of Guest visiting Beru Guest House in providing a Kitchen with Storage & Toilet. The project is ongoing, and will continue its process until it is completed.

### Requirements

All supporting documentation must be in English. Kindly note that the list of requirement can be found in the **Instructions on How to Submit Tender** template, page 5.

### Installation services

* Construction Services

### Delivery Time

Suppliers are required to provide the delivery time frame.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | Hardcore (sand) 150mm Thick | 38 Bags |  |  |
| 2 | 40 kg Porland Cement | 75 Bags |  |  |
| 3 | M12mm Dia Dynabolt with nut and washers | 36 Each |  |  |
| 4 | Form ply 2.4x1.2 | 7 Sheet |  |  |
| 5 | Pine Timber 2x2x6m | 12 Length |  |  |
| 6 | 3” Galvanised Nail | 4 Kg |  |  |
| 7 | 2” Galvanised Nail | 3 Kg |  |  |
| 8 | Damp proof membrane (60x20m) per roll | 1 Roll |  |  |
| 9 | Deformed Reinforcing Bar 10mm Dia | 16 Length |  |  |
| 10 | R6mm Diameter Sitrrup | 9 Length |  |  |
| 11 | Tie Wire | 7 Roll |  |  |
| 12 | Deformed Reinforcing bar 10mm Dia | 13 Length |  |  |
| 13 | R6mm Stirrup in Knock out beam | 2 Length |  |  |
| 14 | Fabric Mesh Wire Reinforcement | 1 Sheet |  |  |
| 15 | Blocks 150x390x150mm in size | 384 nos |  |  |
| 16 | Blocks 100x390x100 (4”) size | 150 nos |  |  |
| 17 | 10 Blades Louver Frame | 2 Pair |  |  |
| 18 | 4 Blades Louver Frame | 1 Pair |  |  |
| 19 | 100x50mm Pine Timber | 3 Length |  |  |
| 20 | SS – Strap | 3 Metre |  |  |
| 21 | M12mm Dyna Bolt with nut and washer | 18 nos |  |  |
| 22 | Gang Nail Plate | 50 nos |  |  |
| 23 | 50x50mm Pine Timber | 8 Length |  |  |
| 24 | 3” Galvanized Nail | 2 Kg |  |  |
| 25 | 100x50mm Pine Timber | 8 Length |  |  |
| 26 | 4” Galvanised Nail | 4 Kg |  |  |
| 27 | 100x50mm Strut and Brace | 2 Length |  |  |
| 28 | 3” Galvanised Nail | 1 Kg |  |  |
| 29 | 75x50mm Pine Timber | 5 Length |  |  |
| 30 | 3” Galvanised Nail | 2 kg |  |  |
| 31 | 150x25mm Pine Timber | 2 Length |  |  |
| 32 | 2” Flat Head Nail | 1 Kg |  |  |
| 33 | 150x25mm Barge Board | 2 Length |  |  |
| 34 | Hardboard Ceiling Masonite Sheet | 5 Sheet |  |  |
| 35 | Panel Pin | 1 Kg |  |  |
| 36 | 150x50mm Pine Timber | 11 Length |  |  |
| 37 | 2” Flat Head Nail | 2 Kg |  |  |
| 38 | 200x50mm Pine Timber | 4 Length |  |  |
| 39 | 4” Galvanised Nail | 3 Kg |  |  |
| 40 | 250x50mm Dakua timber | 1 Length |  |  |
| 41 | 200x50mm Pine Timber | 2 Length |  |  |
| 42 | 3” Galvanised Nail | 1 Kg |  |  |
| 43 | Exterior New Door as per Design required | 2 Each |  |  |
| 44 | New Counter Shelves | 2 Each |  |  |
| 45 | New Table with Shelves | 1 nos |  |  |
| 46 | 100mm Butt Hinges | 4 Each |  |  |
| 47 | Plain Mortice lock | 2 Each |  |  |
| 48 | Corrugated Zincalume Sheet 15 Feet | 8 Sheet |  |  |
| 49 | Roofing nail with rubber 3” | 2 Pkt |  |  |
| 50 | Sisalition Alum Foil | 1 Roll |  |  |
| 51 | Chicken Wire | 1 Roll |  |  |
| 52 | Alum Gutter with bracket (2.4m in length) | 3 Length |  |  |
| 53 | Gutter bracket | 10 nos |  |  |
| 54 | 10mm Diameter PVC Downpipe | 1 Length |  |  |
| 55 | 100mm PVC clips | 3 nos |  |  |
| 56 | 100mm Diameter bend | 2 nos |  |  |
| 57 | 100mm diameter tee | 1 nos |  |  |
| 58 | 15mm PVC pipe with clips | 2 Length |  |  |
| 59 | 25mm PVC pipe with clips | 5 Length |  |  |
| 60 | 15mm Diameter Bend | 2 Each |  |  |
| 61 | 15mm Diameter Tee | 2 Each |  |  |
| 62 | 15mm Diameter Male adaptor | 2 each |  |  |
| 63 | 15mm Diameter female adaptor | 2 each |  |  |
| 64 | 25mm Diameter bend | 2 each |  |  |
| 65 | 25mm Diameter Tee | 2 each |  |  |
| 66 | 25mm Diameter male adaptor | 2 each |  |  |
| 67 | 25mm diameter female adaptor | 2 each |  |  |
| 68 | 32mm diameter PVC pipe | 1 length |  |  |
| 69 | 32mm diameter bend | 2 each |  |  |
| 70 | 32mm diameter tee | 2 each |  |  |
| 71 | 32x65mm reducer | 1 each |  |  |
| 72 | 65mm diameter PVC pipe | 1 length |  |  |
| 73 | 65mm diameter bend | 2 nos |  |  |
| 74 | 65mm diameter tee | 2 nos |  |  |
| 75 | Single sink unit | 1 each |  |  |
| 76 | 15mm swing tap | 1 nos |  |  |
| 77 | 15mm hose flex | 1 nos |  |  |
| 78 | 15mm cock valve | 1 nos |  |  |
| 79 | 32mm S trap | 1 nos |  |  |
| 80 | Plug and waste | 1 nos |  |  |
| 81 | 15 mm male adaptor | 6 nos |  |  |
| 82 | 32mm female adaptor | 1 nos |  |  |
| 83 | 200mm Block | 90 nos |  |  |
| 84 | Mesh Wire | 1 sheet |  |  |
| 85 | Rod 12mm Diameter 6m | 1 length |  |  |
| 86 | Rod 16mm Diameter 6m | 2 length |  |  |
| 87 | Qualified Electrician for investigating and installing new electrical appliances to conduct testing on site from a 1 KW solar kit | 1 each |  |  |
| 88 | 300x300mm non slip ceramic tile | 133 pieces |  |  |
| 89 | Adhesive CTF 20kg | 2 bag |  |  |
| 90 | Grout 2kg/pkt | 2 pkt |  |  |
| 91 | Acrylic Sealer 4 litre | 2 tin |  |  |
| 92 | Semi-Gloss 4 litre | 2 tin |  |  |
| 93 | Super enamel 4 litre | 4 tin |  |  |
| 94 | Acrylic sealer undercoat 4L | 4 tin |  |  |
| 95 | Roller brush complete with tray | 2 set |  |  |
| 96 | 4” hand paint brush | 2 nos |  |  |
| 97 | Narrow surface 0-300mm girth | 65 meter |  |  |
| 98 | Wood primer 4L | 1 tin |  |  |
| 99 | Semi-Gloss 4L | 1 tin |  |  |
| 100 | 36x6” louver glass clear | 49 nos |  |  |
| 101 | Security wire meshing to external opening | 2 sheet |  |  |
| 102 | 50x50mm timber battens | 1 length |  |  |
| 103 | 2” galvanised nail | 1 kg |  |  |
| 104 | Flyscreen sheet | 1 roll |  |  |
| 105 | Hard core imported 150mm thick | 24 bag |  |  |
| 106 | Portland cement 40kg | 56 bag |  |  |
| 107 | Formply for framework | 4 sheet |  |  |
| 108 | 2” flat head nail | 1 pkt |  |  |
| 109 | 50x50mm pine timber for formwork | 2 length |  |  |
| 110 | 200x25mm pine timber for formwork | 2 length |  |  |
| 111 | 3” flat head nail for formwork | 1 pkt |  |  |
| 112 | Damp proof membrane (60x2m wide) 0.2mm thick | 1 roll |  |  |
| 113 | Deformed 12mm diameter reinforcing bar in footing | 5 length |  |  |
| 114 | Deformed 10mm diameter reinforcing bar in footing | 12 length |  |  |
| 115 | R6mm diameter stirrup ties at 400 c-c | 2 length |  |  |
| 116 | R6mm diameter stirrup ties at 400 c-c in overhead tank | 6 length |  |  |
| 117 | Deformed 12mm starter bar including laps | 17 length |  |  |
| 118 | Mesh wire (5.4x2.4m) | 2 sheet |  |  |
| 119 | Tie wire 15m/roll | 10 nos |  |  |
| 120 | 4 blades louver frame | 2 pair |  |  |
| 121 | 400x200x200mm block (8”) | 819 nos |  |  |
| 122 | 100x50mm Pine Timber for top plate | 2 length |  |  |
| 123 | 4” concrete nail | 1 kg |  |  |
| 124 | 50x50mm Pine timber | 4 length |  |  |
| 125 | 100x50mm pine timber | 5 length |  |  |
| 126 | 4” nail | 2 pkt |  |  |
| 127 | 3” nail | 2 pkt |  |  |
| 128 | 100x50mm pine timber | 3 length |  |  |
| 129 | 75x50mm pine timber | 4 length |  |  |
| 130 | 200x20mm pine timber | 1 length |  |  |
| 131 | 2” nail | 2 pkt |  |  |
| 132 | 200x20mm pine timber | 1 length |  |  |
| 133 | Masonite 2.4x1.2/sheet | 2 sheet |  |  |
| 134 | 50x20mm pine timber for scotia | 3 length |  |  |
| 135 | 20mm diameter incoming PVC pipe for water reticulation | 2 length |  |  |
| 136 | 20mm diameter bend | 2 length |  |  |
| 137 | 20mm diameter tee | 4 nos |  |  |
| 138 | 20mm diameter male adaptor | 4 nos |  |  |
| 139 | 20mm diameter female adaptor | 4 nos |  |  |
| 140 | 20x15mm reducer | 2 nos |  |  |
| 141 | WC pan suit with P – trap | 2 nos |  |  |
| 142 | Pan collar | 2 nos |  |  |
| 143 | Flushing cistern dual system | 2 nos |  |  |
| 144 | Pan seat and lid | 2 nos |  |  |
| 145 | 15mm dia hose flex | 2 nos |  |  |
| 146 | 15mm dia cock valve | 2 nos |  |  |
| 147 | 15mm female adaptor | 1 nos |  |  |
| 148 | 15mm male adaptor | 2 nos |  |  |
| 149 | Tread tape | 3 nos |  |  |
| 150 | Solvent cement 500ml | 2 nos |  |  |
| 151 | Wash hand basin complete with brackets (small size) | 2 nos |  |  |
| 152 | 15mm tap | 2 nos |  |  |
| 153 | 15mm male adaptor | 2 nos |  |  |
| 154 | 15mm female adaptor | 2 nos |  |  |
| 155 | 32mm S – Trap (same size to hand basin) | 2 nos |  |  |
| 156 | 32mm female adaptor | 2 nos |  |  |
| 157 | 32mm male adaptor | 2 nos |  |  |
| 158 | Plug and waste | 2 nos |  |  |
| 159 | 32mm PVC pipe | 1 length |  |  |
| 160 | 400x200x200mm block | 414 nos |  |  |
| 161 | 40kg Portland cement | 52 bag |  |  |
| 162 | F62 fabric mesh wire (6x2m/sheet) | 2 sheet |  |  |
| 163 | Rod 16mm | 18 length |  |  |
| 164 | 150x25mm pine timber | 5 length |  |  |
| 165 | 100x50mm pine timber | 2 length |  |  |
| 166 | 4” flat nail | 1 pkt |  |  |
| 167 | 3” flat nail | 1 pkt |  |  |
| 168 | 20mm thick concrete block | 264 nos |  |  |
| 169 | F62 fabric mesh wire 6x2.4m/sheet | 1 sheet |  |  |
| 170 | Rod 12mm diameter 6m | 6 length |  |  |
| 171 | Rod 16mm diameter 6m | 5 length |  |  |
| 172 | 4” flathead nail | 1 kg |  |  |
| 173 | 3” flathead nail | 1 kg |  |  |
| 174 | Roller brush set | 1 nos |  |  |
| 175 | Paint hand brush 3” | 1 nos |  |  |
| 176 | Undercoat 4L | 1 tin |  |  |
| 177 | Semi-gloss 4L | 1 tin |  |  |
| 178 | 2” paint hand brush | 1 nos |  |  |
| 179 | 24x6 obscure glass blade | 8 nos |  |  |