**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**PROCUREMENT OF CONSTRUCTION MATERIALS FOR 8 DISASTER PROJECTS**

**Procurement No.:** 09-G014-24

## Specification

### Background

### OB via its Disaster Risk Management Unit is undergoing the procurement of construction materials for 8 disaster projects. These disaster projects are situated at outer islands consisting of building and seawall projects.

### To execute these under the formal procurement procedure, OB had sought the approval for utilizing the open competitive method under a reduced tender period of 10 working days for the urgent need of these to be implemented before end of this year.

For the delivery arrangement, OB is anticipated to work with the identified communities on the delivery plan made by the supplier.

### Requirements

* All supporting documentation must be in English.
* Should Provide a clear quote(s) and follow every instruction stated in this template starting from submission to delivering of goods.

Please note that the list of requirements can be found in the ***Instructions on How to Submit a Quotation*** template, page 5.

### Installation services

* Not applicable in this procurement

**Delivery Time**

* OB will be handling the delivery of this good to the community.

## Description of the Goods

*Here, list all items to be Tendered.*

1. **Construction materials for KUC Banaba Church**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | T/Price Quotation |
| 40 Kg Portland Cement | 122 | Bags |  |  |
| 12mm dia H.D bolt with nut and washers | 31 | Each |  |  |
| 200×200×400mm Block | 726 | nos |  |  |
| Formply 2.4×1.2m per sheet | 7 | Sheet |  |  |
| Pine Timber 2×2×5.8m | 79 | Length |  |  |
| Nail 4" | 35 | Kg |  |  |
| Nail 2" | 11 | Kg |  |  |
| Polythene | 1 | Roll |  |  |
| Deformed 10mm diameter reinforcing bar | 30 | Length |  |  |
| Reinforcing rod 6mm diameter stirrup | 16 | Length |  |  |
| Deformed 12mm reinforcing bar starter bar | 19 | Length |  |  |
| Deformed 10mm reinforcing bar in bond beam | 24 | Length |  |  |
| Reinforcing rod 6mm diameter | 4 | Length |  |  |
| Mesh Wire (2.3×5.8×2mm) | 6 | Sheet |  |  |
| Tie Wire | 20 | Roll |  |  |
| Triplegrip Steel Connector | 22 | Each |  |  |
| Louver Frame 10 Blades | 21 | Pair |  |  |
| Laminated Pine Timber 100×50×5800 | 8 | Length |  |  |
| U bracket bowmac post | 4 | Each |  |  |
| Pine Timber 4×2×5.8m | 46 | Length |  |  |
| Pine Timber 3×2×5.8m | 29 | Length |  |  |
| Pine Timber 8×1×5.8m | 16 | Length |  |  |
| S Strap for diagonal bracing | 47 | Meter |  |  |
| Flat Head Nail 1" | 1 | Kg |  |  |
| Marine Plywood 2.4×1.2×12mm thick | 11 | Sheet |  |  |
| Nail 3" | 14 | Kg |  |  |
| Masonite Sheet 2.4×1.2 | 17 | Sheet |  |  |
| Nail Pin | 5 | Kg |  |  |
| Dakua Timber 8×2×5.8m | 12 | Length |  |  |
| Nail 1" | 3 | Kg |  |  |
| 100mm butt brass hinges with screw | 3 | pair |  |  |
| Rebated mortice lock complete with handles and keys | 2 | each |  |  |
| 100mm barrel bolt with screw | 2 | each |  |  |
| Colorbond corrugated roofing sheet 15 feets | 36 | Sheet |  |  |
| Colorbond roofing sheets 5fts | 10 | Sheet |  |  |
| Roofing screw 3" with rubber washer | 1,108 | pcs |  |  |
| Sisalation aluminium foil (30×1m) | 4 | Roll |  |  |
| Chicken wire mesh (30×1m) | 4 | Roll |  |  |
| Colorbond Aluminium ridge cap | 7 | Sheet |  |  |
| Colorbond Aluminium roof flashing | 8 | Sheet |  |  |
| Flat head nail 2" | 2 | Kg |  |  |
| Colorbond aluminium gutter with bracket | 16 | Sheet |  |  |
| P50pcs/pktop rivet | 4 | pkt |  |  |
| Outlet to gutter 100mm diameter | 2 | each |  |  |
| 100mm dia PVC Pipe | 6 | Length |  |  |
| 100mm pvc clips | 3 | each |  |  |
| 100mm dia bend | 8 | each |  |  |
| 100mm dia tee with access cap (Screwed) | 2 | each |  |  |
| Switchboard complete with circuit breaker, wiring and connections | 1 | each |  |  |
| Conduit pipe 15mm | 2 | length |  |  |
| 15mm clips | 3 | each |  |  |
| Circuit wire for powerpoint 2.5mm | 30 | m |  |  |
| 1.5mm circuit wire | 160 | m |  |  |
| 4ft led fluorescent light | 10 | each |  |  |
| Pendant light complete with holder | 2 | each |  |  |
| Ceiling fan 48" complete with switch | 8 | each |  |  |
| Power point double | 2 | each |  |  |
| mounting | 4 | each |  |  |
| two-way switch way single | 2 | each |  |  |
| Non slip ceramic tile 300×300mm (17pcs/box) | 48 | box |  |  |
| adhesive CTF 20Kg | 39 | Bag |  |  |
| 20kg Grout | 2 | Bag |  |  |
| Acrylic sealer undercoat 4 litre | 19 | Tin |  |  |
| Semi gloss 4 Litre | 11 | Tin |  |  |
| Enamel undercoat 4 litre | 10 | Tin |  |  |
| Super enamel 4 litre | 11 | Tin |  |  |
| Varnish 4 Litre | 2 | Tin |  |  |
| Pink Primer 4 litre | 3 | Tin |  |  |
| 4" Hand brush | 4 | each |  |  |
| 2" Hand brush | 4 | each |  |  |
| 4" set roller brush with tray | 5 | set |  |  |
| Louver clear glass 36"×6" | 220 | each |  |  |
| SS mesh security 2×1m/sheet | 10 | sheet |  |  |
| U nail 1.5 - 2 inches | 3 | kg |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction materials for Terikiai Maneaba, Tab North**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| D10 dia rebar 6m (3/8) | 60 | Length |  |  |
| D16 dia rebar 6m (5/18) | 30 | Length |  |  |
| External plywood 12mm, 2.4m, 1.2m (1/2) | 7 | Sheet |  |  |
| Formply 17mm, 2.4, 1.2 (5/8) | 10 | Sheet |  |  |
| M12 + 230 bolt & nut & washer galvanized (3/4) | 40 | each |  |  |
| Jolthead galvanize nails (4) | 30 | Kg |  |  |
| Flat head galvanize nails 1(1/2) | 4 | Kg |  |  |
| Flathead galvanize nails (2) | 7 | Kg |  |  |
| Jolthead galvanize nails (2) | 4 | Kg |  |  |
| Jolthead galvanuze nails (3) | 7 | Kg |  |  |
| Nails panel pin 25" flathead | 6 | Kg |  |  |
| Polytheno 0.9m + 60m | 6 | Rolls |  |  |
| Portland Cement 40 Kg | 275 | bags |  |  |
| Punched strap galv 25×1m×40 | 6 | Coil |  |  |
| R6 dia rebar × 6m (1/4) | 50 | Length |  |  |
| Ridge cap 24 gauge 2.4m | 17 | Length |  |  |
| Roofing Sheets Zinacalume 10 fts | 7 | Sheets |  |  |
| Roofing Sheets Zinacalume 12 fts | 12 | Sheets |  |  |
| Roofing Sheets Zinacalume 15 fts | 34 | Sheets |  |  |
| Roofing Sheets Zinacalume 6 fts | 14 | Sheets |  |  |
| Roofing Sheets Zinacalume 8 fts | 40 | Sheets |  |  |
| Roofing Sheets Zinacalume 9 fts | 24 | Sheets |  |  |
| Roofing nails 65mm with washier | 25 | Kg |  |  |
| Sisalation paper 1.2×40m | 10 | Roll |  |  |
| Mesh Wire 5m×2.4m | 16 | Sheet |  |  |
| Tie wire 1 Kg | 21 | Coils |  |  |
| Timber Pine 100×50×6m (4"×2"×6m) | 63 | Length |  |  |
| Timber Pine 150×50×6m (6"×2"×6m) | 40 | Length |  |  |
| Timber Pine 200×25×6m (8"×1"×6m) | 16 | Length |  |  |
| Timber Pine 200×50×6m (8"×2"×6m) | 30 | Length |  |  |
| Timber Pine 50×50×6m (2"×2"×6m) | 47 | Length |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction materials for TTHC Chapel**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| Radiata pine 200x50mm in 6m long dressed for frames | 46 | length |  |  |
| Radiata pine 100x50mm in 6m long | 257 | length |  |  |
| 0.55mm BMT colorbond ultra (in corrugated) (15 feet) | 136 | sht |  |  |
| 0.55 BMT Colorbond ridge capping | 44 | pcs |  |  |
| 0.55 BMT Clourbond eaves guttering with bracket as necessary | 28 | pcs |  |  |
| Louver frame - 8 blade | 37 | no |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction materials for KUC Buariki Maneaba, North Tarawa**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| Pine Timber 8×2×6m | 20 | Length |  |  |
| Pine Timber 6×2×6m | 62 | Length |  |  |
| Pine Timber 3×2×6m | 44 | Length |  |  |
| Corrugated Zinc roofing sheet 15 ft | 163 | Sheets |  |  |
| Roofing Nails | 48 | Kg |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **Vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction materials for KUC Kamauanea Maneaba**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| Pine Timber 8×2×6m | 20 | Length |  |  |
| Pine Timber 6×2×6m | 62 | Length |  |  |
| Pine Timber 3×2×6m | 44 | Length |  |  |
| Corrugated Zinc roofing sheet 15 ft | 163 | Sheets |  |  |
| Roofing Nails | 48 | Kg |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. Construction materials for KUC Tekatana seawall

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| Cement 40Kg | 850 | Bags |  |  |
| Geotextile 100m/roll | 1 | Roll |  |  |
| Sandbag | 1674 | pcs |  |  |
| Formply sheet 3/4" | 9 | sheets |  |  |
| Timber frame 100×50mm | 15 | Length |  |  |
| Nails 4" | 5 | Kg |  |  |
| Nails 3" | 2 | Kg |  |  |
| Nails flat 1 1/2" | 2 | Kg |  |  |
| PVC Pipe 100mm | 2 | Length |  |  |
| Hand Saw | 1 | nos |  |  |
| Tape measure 50 mtr | 1 | nos |  |  |
| Tape measure 8 mtr | 1 | nos |  |  |
| Bench Bar | 1 | nos |  |  |
| Shovels | 15 | pcs |  |  |
| Hammer | 1 | pcs |  |  |
| Wheelbarrow | 4 | nos |  |  |
| Crow Bar | 1 | pcs |  |  |
| **Total cost** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |


1. **Construction materials for CPPL Bairiki seawall**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Quantity** | **Unit** | **Price Quotation** | **T/Price Quotation** |
| Cement 40Kg | 393 | bags |  |  |
| Geotextile | 1 | roll |  |  |
| Sandbag | 813 | pcs |  |  |
| PVC pipe 100mm diam | 1 | Length |  |  |
| Formply Sheets 3/4" | 7 | sheets |  |  |
| Timber 100×50mm | 21 | length |  |  |
| Nail 4" | 7 | Kg |  |  |
| Nail 3" | 4 | Kg |  |  |
| Nail 1 1/2" flat head | 3 | Kg |  |  |
| Tape measure 50 mtr | 1 | nos |  |  |
| Tape measure 8 mtr | 2 | nos |  |  |
| Handsaw | 4 | nos |  |  |
| Crow bar | 4 | nos |  |  |
| Claw Hammer | 10 | nos |  |  |
| Shovels | 15 | nos |  |  |
| Wheel barrow | 4 | nos |  |  |
| Gloves | 21 | pairs |  |  |
| Safety Glasses | 21 | nos |  |  |
| Rubber boot | 10 | pairs |  |  |
| Vest | 21 | nos |  |  |
| Helmet | 21 | nos |  |  |
| **Total cost** |  |  |  |  |
| **other charges if any** |  |  |  |  |
|  |  |  |  |  |
| **vat** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction material for disaster projects**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Specification** | **Quantity** | **Price Quotation** | **T/Price Quotation** |
| Sandbag | Either option 1 | 1500 |  |  |
|  | **Total cost** |  |  |  |
|  | **other charges if any** |  |  |  |
|  |  |  |  |  |
|  | **vat** |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| **Item** | **Specification** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Sandbag | OR option 2 | 1,500 |  |  |
|  | **Total cost** |  |  |  |
|  | **other charges if any** |  |  |  |
|  |  |  |  |  |
|  | **vat** |  |  |  |
|  | **Total cost (vat inclusive)** |  |  |  |

Option 1:



Option 2:

