**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No: 46-G014-25**

## Specification

### Background

This project is to support efficiency of fuel delivery on the outer island from time to time

### Requirements

All supporting documentation must be in English.

* Please refer to **template 2 and 5** for the full information of the requirements and critieria

### Installation services

To be delivered in complete.

### Delivery Time

6 Months

## Description of the Goods

*Here, list all items to be Tendered*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | Aviation Tanker Truck (Bridger)   * 17,000 litre two-compartment tank on a 6x2 Isuzu * Refuel International Fuelling Module with single Underwing and Overwing Hose-reels * 1135 Litre per minute Filter Monitor * Gorman Rupp PD product Pump all enclosed within canopy with a roller shutter door * Bottom Loading of the refueller tank rate of up to 1,500 lpm and is linked to the overfill protection system and if activated, all loading shuts off at SFL. * Overfill Protection is by way of the tank-top primary High probe & secondary / High-High probe. * EI 1596 Specification Design and Construction of Aviation Fuel Filter Vessels. * EI/JIG Standard 1530 Quality assurance requirements for the manufacture, storage and distribution of aviation fuel to airports. | 1 |  |  |