**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No: 29-G008-25**

## Specification

### Background.

This procurement is for a new bucket truck intended to replace the old and currently the only existing bucket truck in operation. The existing vehicle is essential for high-voltage maintenance and repair works carried out by the Electricity Division. When the current bucket truck is out of service, staff are unable to perform these critical operations, resulting in interruptions to maintenance and potential disruptions to power services. The acquisition of a new bucket truck will therefore ensure operational continuity and maintain a reliable power supply.

### Requirements

All supporting documentation must be in English. Final quote should be in AUD and CIF Kiritimati. The following documents should be submitted. Failure to provide will result in disqualifying the tenderer.

1. Cover letter
2. Valid Business Registration
3. Update and Latest Tax Clearance from Tax office
4. Valid Operational license from Local Council (if appliable)
5. Signed copy of the Certificate for Compliance Form. Refer to ITT Template No.8 for a copy of the certificate for compliance form.
6. Delivery schedule, Specification compliance and other technical requirements (Refer to template 5 for further information)
7. Financial Proposal including **Quotation** (Complete quotation in **AUD and CIF Kiritimati** indicating a clear financial proposal) and **Financial annual reports**

### Installation services

The Ministry (MLPID) through the Electrical Division have a capacity to install the project.

### Delivery Time

To be arrived at Kiritimati Island in Early 2026.

## Description of the Goods

**To Purchase the Following Equipment:**

Make/Model: 2015 Isuzu FRR500 AMT 4x2 Truck

Fitted With: Versalift VST40 I EWP

Registration: HYW721

Stock Number: 1061

**Vehicle Specifications:**

Vehicle Manufacturer: ISUZU

Vehicle Model: F Series

Engine: GVM: 10,400kg

TRANS: 6-GEAR AUTO GCM:

R/Axle: 7,700kg

Tare: 7,500kg

**Boom Specifications:**

Model: VST40

Max Working Radius: 9.50m

Manufacturer: Versalift

Working Height: 14.20m

Boom Style: Articulating/telescopic Platform Height (ground to bucket floor): 12.20m

Auto Stow: Insulation Category: C (46Kv)

Bucket Capacity (SWL): 227kg

Bucket Lift: Yes

Outrigger: Bucket Rotation: Yes