**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **RFQ-27-G003-22**

## Specification

### Background

This tender is to supply the Ministry of Infrastructure and Sustainable Energy (MISE) Civil Engineering Division with the following Goods:

|  |  |  |  |
| --- | --- | --- | --- |
| **Ref** | **Description** | **Quantities** | **Unit** |
| 1 | Cement 40kg | 484 | bags |
| 2 | Sandbag | 2428 | pcs |
| 3 | Shovels | 5 | pcs |
| 4 | Wheel barrow | 2 | Pcs |
| 5 | Cost and Freight Abemama |  |  |

The tools/materials are urgently needed to repair work of the seawall to avoid further problem that might occur later. Tanimaniku Seawall requires patch work to replace the damaged revetment and the toe.

The quote must include VAT, C/F and handling services in Abemama.

### Requirements

All supporting documentation must be in English.

Tenders must include the following:-

* Catalog, Manuals, photos, brochures on the products and packaging.
* Technical specifications, etc.
* On-line training and instructions on the application of the mix.

<list other general requirements>

### Installation services

<insert related services>

### Delivery Time

<insert requested delivery time, if general, otherwise in the table below>

## Description of the Goods

*Refer to* ***Annex B*** *attached herewith for list all items to be Tendered.*

*(This part may be replaced by a proprietary Supplier description)*

***Annex B:***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ref** | **Description** | **Specification** | **Quantities** | **Unit** |
| 1 | Cement 40kg | Portland (GP) | 484 | bags |
| 2 | Sandbag | Size 300x150x100 (small bag) | 2428 | pcs |
| 3 | Shovels | Long Shovel (sharp end) | 5 | pcs |
| 4 | Wheel barrow | Normal Wheel Barrow | 2 | Pcs |