**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **50-G003-22**

## Specification

### Background

### The supply of the signage is being managed by the Kiribati Utilities Reform Programme and is funded by the New Zealand Ministry of Foreign Affairs and Trade.

### The signage will be used by the Public Utilities Board which supplies water, sanitation and electricity services to South Tarawa in the Republic of Kiribati, the Ministry of Line and Phoenix Islands Development which provides the same to Kiritimati Island and the Ministry of Infrastructure and Sustainable Energy which provides the same to the outer islands.

This is a one-off contract although the Procuring Entity may order additional signs in future years. If so, the Procuring Entity will negotiate a new price using the price quoted in this contract as a basis.

### Requirements

For the signs in English, the signage shall comply with Australian/New Zealand Standards or International Standards Organisation Safety Sign Standards. The supplier shall quote the Standard(s) to which its signage conforms. A mix of Standards is acceptable. For the signs in i-Kiribati, the signs shall comply with these Standards as closely as practical.

The signs shall be made from the materials listed in the Description of Goods, and shall be approximately the dimensions listed in the Description of Goods. In the case of a particular sign being readily available in an alternative material or similar size, the supplier, may nominate this alternative material and will not be penalised for doing so.

One set of signs shall be in English on one set of signs shall be in i-Kiribati. Translations have been provided.

All supporting documentation must be in English.

### Packing, Shipment and Acceptance

The signs shall be packed and shipped as follows:

* Packed in protective and waterproof wrapping.
* Assembled in separately labelled packages (labels to be PUB, MISE, MPLID and Electricity, Water making 3 x 2 = 6 packages – see Description of Goods).
* Shipped by container to the Port of Betio or by Air Freight to Bonriki International Airport depending upon the size and weight of the packages.
* Part-orders may be shipped as the Goods become available with a maximum of four shipments in total being made.
* The Goods will be collected by a KURP representative and checked before being individually accepted within four days of arrival.
* Once accepted payment will be made for the Goods individually accepted.

### Delivery Time

The contract requires the Goods to be delivered either to the Port of Betio or to the Bonriki International Airport at the Supplier’s discretion. The Goods may be delivered in one or up to four separate packages, and the Supplier will be paid accordingly. All goods must be delivered within six months of the contract effective date.

## Description of the Goods

The following table describes the signs and quantities to be provided.

* PUB: Public Utilities Board
* MLPID: Ministry of Line and Phoenix Islands Development
* MISE: Ministry of Infrastructure and Sustainable Energy

**English Order**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Description** | **Sign** | **Quantity** | | |
| **PUB** | **MLPID** | **MISE** |
| **Electricity** | | | | | |
| 1 | Entrance  140mmx400mm  Polypropylene  AUD48.26 |  | 5 | 5 | 2 |
| 2 | Exit  Luminous  180mmx450mm  Self-Adhesive Vinyl  AUD 54.49 |  | 5 | 5 | 2 |
| 3 | Exit  Luminous  180mmx350mm  Metal  AUD 75.50 |  | 5 | 5 |  |
| 4 | Authorised Employees Only  254mmx356 mm  Self-Adhesive Vinyl  90mmx125mm  AUD 47.96 |  | 10 | 5 | 10 |
| 5 | Authorised Employees Only  225mmx300mm  Metal  AUD 32.85 |  | 5 | 5 |  |
| 6 | Danger – High Voltage  225mmx300mm  Metal  AUD 32.85 |  | 8 | 5 |  |
| 7 | Danger – Do Not Enter  300mmx450mm  Metal  AUD34.77 |  | 5 | 5 |  |
| 8 | Trips Hazards  225x300  Polypropylene  AUD 28.53 |  | 8 | 5 |  |
| 9 | Trips Hazards  250x180  Self-Adhesive Vinyl  AUD 16.86 |  | 5 | 5 | 12 |
| 10 | Buried Cable  450mmx600mm  Polypropylene  AUD129.94 |  | 5 | 5 |  |
| 11 | Buried Electric Cable  450mmx600mm  Metal  AUD 149.79 |  | 10 | 5 |  |
|  | **Water and Wastewater Signs** | | | | |
| 12 | Entrance  140mmx400mm  Polypropylene  AUD48.26 |  | 5 |  | 15 |
| 13 | Exit  Luminous  180mmx450mm  Self-Adhesive Vinyl  AUD 54.49 |  | 5 |  | 15 |
| 14 | Exit  Luminous  180mmx350mm  Metal  AUD 75.50 |  | 5 |  | 15 |
| 15 | Authorised Employees Only  Polypropylene  225x300  AUD 28.53 |  | 5 |  | 30 |
| 16 | Danger – Do Not Enter  300x450  Metal  AUD 34.77 |  | 5 |  | 3 |
| 17 | Trips Hazards  225x300  Polypropylene  AUD 28.53 |  | 5 |  | 2 |
| 18 | Trips Hazards  250x180  Self-Adhesive Vinyl  AUD 16.86 |  | 5 | 5 | 2 |
| 19 | (Construction Work Ahead)  Prepare to Stop Kit  600mmx900mm  Powder Coated Steel  AUD 182.05 |  | 4 | 4 | 2 |
| 20 | (Construction Work Ahead)  Prepare to Stop Sign  1200mmx900mm  Metal  AUD 118.44 |  | 4 | 4 | 4 |
| 21 | (Construction Work Ahead)  Speed Limit 10 Sign  450mmx600mm  Metal  AUD 63.60 |  | 5 | 5 | 4 |
| 22 | Barriers  2.4 m  AUD 148.79 |  | 10 | 5 |  |
| 23 | Cones  Hi-Vis  450mm or 700mm high  PVC  AUD51.60 |  | 10 blue with white band Hi-Vis  20 orange with white band Hi-Vis | 10 blue with white band Hi-Vis  20 orange with white band Hi-Vis | 4 blue with white band Hi-Vis  8  orange with white band Hi-Vis 12 |
| 24 | Printed Barrier Tape  75mmx60m  Polypropylene  AUD32.58 |  | 10 | 10 | 5 |
| 25 | (Trenches)  Deep Excavation  450mmx600mm  Polypropylene  AUD129.94 |  | 4 | 4 | 3 |
| 26 | (Trenches)  Excavation In Progress  450mmx600mm  Polypropylene  AUD60.51 |  | 4 | 4 | 2 |
| 27 | (Trenches)  Construction Site Do Not Enter  450mmx600mm  Polypropylene  AUD60.51 |  | 5 | 5 | 2 |

**i-Kiribati Order**

As above but in i-Kiribati. Translations are listed in the following table. Sign size and/or (preferably) letter size may be adjusted to accommodate the words.

|  |  |
| --- | --- |
| **English** | **i-Kiribati** |
| Entrance | Tabo n Rin |
| Exit | Tabo n Otinako |
| Danger | Kamamate |
| Electrical Hazard | Ko kona ni tiaoki n te Iti |
| Authorised Personnel Only | Ti ibukiia aika a Kariaiakaki |
| High Voltage | Te Iti ae Korakora |
| Do Not Enter | Tai Rin |
| Watch Your Step | Nakonako ma te Taratara Raoi |
| Tripping Hazard | Ko kona ni Kabuanibwai man Baen Waem |
| Cable Buried Below | Iai Te Uaea i Antano |
| Buried Electrical Cable Below | Iai Uaean te Iti i Antano |
| Restricted Area | Te Tabo ae Katabuaki Kawarana |
| Prepare to Stop | Tauraoi n Tei |
| Speed Limit | Tokin te Buti |
| Deep Excavation | Te Mwanono ae Nano |
| Excavation in Progress | E waaki te Keniken |
| Construction Site | Te Tabo ni Kateitei |

## Tenderer’s References

### Relevant similar deliveries carried out in the last three years

Please, provide information on each delivery for which your firm/entity, either individually as a corporate entity or as one of the major companies within an association, was legally contracted.

|  |  |  |
| --- | --- | --- |
| Goods Delivered | Location and Buyer | Contact Details |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |