**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **09-G004-23**

## Specification

### Background

### OB given her role to manage approved requests from the ministerial tour commitment firstly seeking the approval on tendering materials on a reduced tender period. Materials that are required to procure are the construction materials for 4 public toilets on outer Island plus materials which also part of the requests.

### Requirements

* All supporting documentation must be in English.
* Should provide a clear quote(s) and follow every instruction stated in this template starting from submission to delivering of goods.

Please note that the list of requirements can be found in the ***Instructions on How to Submit a Quotation*** template, page 5.

### Installation services

Nil

### Delivery Time

## There will be a charter for delivering materials to outer Islands.

## Description of the Goods

*Here, list all items to be Tendered.*

1. *Materials for Ministerial tour projects*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for Ministerial tour projects** | |  |  |  |
| **Description** | **unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Ceramic tile 300x300mm |  | 51 |  |  |
| CTF |  | 437 |  |  |
| **Total cost** |  |  |  |  |
| **Vat** |  |  |  |  |
| **other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. **Construction materials for 4 public toilets**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Material list for public toilets for Tekarano Abaiang, Tabontebike Abaiang, Abatao North Tarawa and KUC Tekem Maiana** | | |  |  | |
| **Description** | **Unit** | **Qty for 1 project** | **Qty for 4 projects** | **Price Quotation** | **T/Price Quotation** |
| Brick (6 size) | nos | 1173 | 4692 |  |  |
| 40 kg Cement | bag | 141 | 564 |  |  |
| 50x50mm pine timber | length | 2 | 8 |  |  |
| Formply for formwork | sheet | 4 | 16 |  |  |
| 3 nail | kg | 2 | 8 |  |  |
| 4 nail | kg | 2 | 8 |  |  |
| “2” flat head nail | kg | 1 | 4 |  |  |
| 50x50mm pine timber | lengths | 2 | 8 |  |  |
| 200x25mm pine timber | lengths | 2 | 8 |  |  |
| “2” flat head nail for formwork | kg | 1 | 4 |  |  |
| Deformed 12mm diameter reinforcing bar in footing | length | 5 | 20 |  |  |
| Tie wire 15m/roll | nos | 20 | 80 |  |  |
| Deformed 10mm diameter reinforcing bar in footing | length | 12 | 48 |  |  |
| R6mm diameter stirrup ties at 400c-c | length | 2 | 8 |  |  |
| R6mm diameter stirrup ties at 400 c-c | length | 6 | 24 |  |  |
| Deformed 12 mm starter bar including laps | length | 17 | 68 |  |  |
| Mesh wire (5.4x2.4) m | sheet | 2 | 8 |  |  |
| 4 blade louver frame | pair | 2 | 8 |  |  |
| 100x50mm pine for top plate | length | 3 | 12 |  |  |
| “4” concrete nail | pkt | 4 | 16 |  |  |
| 50x50mm pine timber for celling (2x2) | length | 4 | 16 |  |  |
| 100x50mm pine timber for rafter | length | 5 | 20 |  |  |
| 4 nail | pkt | 2 | 8 |  |  |
| 3 nail | pkt | 2 | 8 |  |  |
| 100x50mm pine timber for strut and Brace | length | 3 | 12 |  |  |
| 75x50mm pine timber for strut and Brace | length | 4 | 16 |  |  |
| 200x20mm pine timber Fascial board | length | 2 | 8 |  |  |
| “2” nail | pkt | 2 | 8 |  |  |
| 200x20mm pine timber for Barge Board | length | 2 | 8 |  |  |
| Masonite 2.4x1.2/ sheet | sheet | 2 | 8 |  |  |
| “1” panel pin nail | pkt | 1 | 4 |  |  |
| 20x20mm pine timber for moulded scotia | length | 3 | 12 |  |  |
| 200x50mm pine timber | length | 1 | 4 |  |  |
| 200x50mm pine timber | length | 2 | 8 |  |  |
| ½ inches exterior plywood | sheets | 4 | 16 |  |  |
| 100x50mm pine timber | length | 2 | 8 |  |  |
| Wood glue 750ml | nos | 1 | 4 |  |  |
| Fine sandpaper “1600” | meters | 2 | 8 |  |  |
| 100mm butt brass with screws | each | 4 | 16 |  |  |
| 100mm butt hinger with screw | pairs | 2 | 8 |  |  |
| Plain mortice lock complete with handles and keys | each | 2 | 8 |  |  |
| Plain mortice lock complete with handles and keys | nos | 2 | 8 |  |  |
| Roofing 15 size | sheet | 6 | 24 |  |  |
| Roofing nail with rubber washer | pkt | 1 | 4 |  |  |
| Sysilation alum foil | roll | 1 | 4 |  |  |
| 20mm diameter incoming pvc pipe for water | length | 2 | 8 |  |  |
| 20mm diameter bend | nos | 10 | 40 |  |  |
| 20mm diameter tee | nos | 4 | 16 |  |  |
| 20mm diameter male adaptor | nos | 4 | 16 |  |  |
| 20mm diameter female adaptor | nos | 4 | 16 |  |  |
| Wc pan suit with p-trap | nos | 2 | 8 |  |  |
| 100mm dia pan collar | nos | 2 | 8 |  |  |
| Flushing cistern dual system | nos | 2 | 8 |  |  |
| Pan seat | nos | 2 | 8 |  |  |
| 15mm dia hose flex | nos | 2 | 8 |  |  |
| 15mm dia cock valve | nos | 2 | 8 |  |  |
| 15mm female adptor | nos | 2 | 8 |  |  |
| 15mm male adptor | nos | 2 | 8 |  |  |
| Tread seal tape | nos | 3 | 12 |  |  |
| Solvent cement 500ml | nos | 1 | 4 |  |  |
| Wash hand basin completed with bracket (small size) | nos | 1 | 4 |  |  |
| 15mm bib tap | nos | 1 | 4 |  |  |
| 15 mm male adptor | nos | 1 | 4 |  |  |
| 15mm female adptor | nos | 1 | 4 |  |  |
| 32mm s-trap | nos | 1 | 4 |  |  |
| 32 mm tee | nos | 2 | 8 |  |  |
| 32mm elbow | nos | 2 | 8 |  |  |
| Plug and waste | nos | 2 | 8 |  |  |
| 32mm pvc pipe | length | 1 | 4 |  |  |
| Water tank 1000L | nos | 1 | 4 |  |  |
| 25mm foot valve | nos | 1 | 4 |  |  |
| 25mm male socket | nos | 2 | 8 |  |  |
| 25mm pvc pipe | length | 2 | 8 |  |  |
| 25mm bend | nos | 5 | 20 |  |  |
| 25mm tee | nos | 3 | 12 |  |  |
| 25mm end cap | nos | 2 | 8 |  |  |
| 25mm Union | nos | 2 | 8 |  |  |
| 15mm Union | nos | 4 | 16 |  |  |
| 20mm union | nos | 3 | 12 |  |  |
| 25mm x 20mm reducing bush | nos | 2 | 8 |  |  |
| 25mm x 15mm reducing bush | nos | 2 | 8 |  |  |
| F62 fabric mesh wire (6x2m/sheet) | sheet | 2 | 8 |  |  |
| Rod 16 mm | length | 18 | 72 |  |  |
| 150x25mm pine timber | length | 5 | 20 |  |  |
| 100x50mm pine timber | length | 2 | 8 |  |  |
| 4 nail | pkt | 1 | 4 |  |  |
| 3 nail | pkt | 1 | 4 |  |  |
| Polythene 30x1.2/roll | roll | 1 | 4 |  |  |
| Undercoat 4ltr | tin | 6 | 24 |  |  |
| Semi-gloss 4ltr | tin | 3 | 12 |  |  |
| Roller brush set | nos | 2 | 8 |  |  |
| Paint hand brush “3” | nos | 2 | 8 |  |  |
| Acrylic sealer 4ltr | tin | 4 | 16 |  |  |
| “2” paint hand brush | nos | 2 | 8 |  |  |
| 24”x”6 (710mm x 150mm) obscure glass blade | pcs | 8 | 32 |  |  |
| Gothic mesh | sheet | 1 | 4 |  |  |
| U nail 1.5 inch | kg | 1 | 4 |  |  |
| **Total cost for 1 project** |  |  |  |  |  |
| **Total cost for 4 Projects** |  |  |  |  |  |
| **vat** |  |  |  |  |  |
| **other charges if any** |  |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |  |