**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**PROCUREMENT OF MATERIALS FOR 8 DISASTER PROJECTS**

**Procurement No.:** **09-G006-23**

## Specification

### Background

### OB every year always received requests in the form of letters and phone calls from the public, schools, churches, and villages communities for their disaster related issues. These requests are attended, inspected by MISE as technical arms of OB, prioritized before being approved, procured and implemented.

This next lots of procurement contains eight (8) beneficiaries namely;

1. KUC Biikati Church Project - Butaritari
2. Abaiang Maneaba Seawall Maintenance Project - Betio
3. KUC Buota Residential House Project – North Tarawa
4. Kuuma Church Project – Butaritari
5. Special School New Mass Concrete Seawall Project - South Tarawa
6. St Iotebwa New Mass Concrete Seawall Project – South Tarawa
7. Taunibong Primary School Maneaba Project –
8. Ueen te Rotario New Mass Concrete Seawall Project

By nature, the seawall projects are matter of urgency to other disaster related requests. As per the above list, 50% of the approved projects are seawall projects. In terms of delivery of the procured projects’ materials, the OB for efficiency and one-off delivery reasons often resorted to vessel charter when normal run by shipping companies is not available.

### Requirements

* All supporting documentation must be in English.
* Should Provide a clear quote(s) and follow every instruction stated in this template starting from submission to delivering of goods.

Please note that the list of requirements can be found in the ***Instructions on How to Submit a Quotation*** template, page 5.

### Installation services

* Not applicable in this procurement

**Delivery Time**

## There will be a charter for delivering materials to outer Islands.

## Description of the Goods

*Here, list all items to be Tendered.*

1. ***KUC Bikaati Church Project***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for KUC Bikaati church Project at Butaritari island** | |  |  |  |
| **Description** | **Unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Portland cement 40 Kg | Bags | 110 |  |  |
| Polythene dam Proof membrane (60m x 2m wide) 0.2mm thick | Roll | 1 |  |  |
| Tire wire (15mtrs) | Coil | 3 |  |  |
| Formply 3/4 thicks | Sheet | 11 |  |  |
| Timber pine 100 x 50mm in 6m long | Length | 5 |  |  |
| Timber pine 50 x 50mm in 6m long | Length | 3 |  |  |
| D10mm dia reinforcing steel (6m Length) deform | Length | 24 |  |  |
| D6mm dia reinforcing steel (6m Length) smooth | Length | 20 |  |  |
| Reinforcing mesh SL102 size:6mx2.4m wide (200x200x10) | Sheet | 6 |  |  |
| 200mm thick block | No. | 90 |  |  |
| Radiata pine 200x25mm in 6m long timber louvre Dressed | Length | 12 |  |  |
| Radiata pine 100x50mm in 6m long to be dressed | Length | 41 |  |  |
| Radiata pine 50x50mm in 6m long to be dressed | Length | 51 |  |  |
| Radiata pine timber 75x50mm in 6m Length to be dressed (new purlin) | Length | 20 |  |  |
| Radiata pine 50x25mm in 6m long door batten | Length | 51 |  |  |
| Radiata pine 50x20mm in 6m long skirting | Length | 2 |  |  |
| Radiata pine 20x20mm in 6m long Quarter round | Length | 14 |  |  |
| Stop ends | No. | 4 |  |  |
| Gutter 2.4m colorbond | No. | 25 |  |  |
| Gutter bracket colorbond | No. | 72 |  |  |
| Outlet to gutter | No. | 2 |  |  |
| Silicon Gun | No. | 2 |  |  |
| Rivert(100 No. / Pkt) | Pkt | 3 |  |  |
| Roof and plumbing Silicon tube | tube | 8 |  |  |
| Rivert Gun | Pkt | 2 |  |  |
| Colorbond corrugated roofing sheet 15 feet | Sheet | 36 |  |  |
| Colorbond corrugated roofing sheet 12 feet | Sheet | 18 |  |  |
| Colorbond corrugated roofing sheet 10 feet | Sheet | 28 |  |  |
| Colobond ridge cap 2.4 m in Length | Pcs | 7 |  |  |
| Colorbond hip cap 2.4m in Length | Pcs | 8 |  |  |
| Syslalation 20x1.5m/ Roll | Roll | 6 |  |  |
| Colorbond roof flashing | Sheet | 10 |  |  |
| 2075x814x40mm external solid core door | No. | 1 |  |  |
| 2070x800x40mm External solid core door. | No. | 1 |  |  |
| 2070x450x40mm External solid core door. | No. | 1 |  |  |
| Steel hinges with screws.100mm | No. | 3 |  |  |
| Rebated mortices lock complete with handles and keys. | No. | 1 |  |  |
| 5 blade louver frame (anodised aluminum with black plastic clips & handle | No. | 2 |  |  |
| 6 blade louver frame (anodised aluminum with black plastic clips & handle | Pr | 1 |  |  |
| 10 blade louver frame (anodised aluminum with black plastic clips & handle | Pr | 30 |  |  |
| 150mm barrel bolts with screws. | No. | 2 |  |  |
| Louver glass 36" | each | 355 |  |  |
| 300x300mm non slip ceramic floor tile on adhesive backing @ 15pc/Box White | Box | 63 |  |  |
| 300x300mm non slip ceramic floor tile on adhesive backing @ 15pc/Box Blue | Box | 12 |  |  |
| CTF Adhesive for ceramic tiles @ 20Kg/bag | Bags | 64 |  |  |
| Tile spacer 2mm @ 100Pcs/Pkt | Pkt | 5 |  |  |
| Grout @ 20Kg/Pkt | Pkt | 2 |  |  |
| plywood 20mm thick | Sheet | 6 |  |  |
| masonite 1.2x2.4 | Sheet | 52 |  |  |
| undercoat enamel 4ltr | Tins | 9 |  |  |
| semi gloss 4ltr | Tins | 9 |  |  |
| Hulux acrylic sealer 4 ltr | Tins | 9 |  |  |
| Roller brush 9" + tray | Tins | 3 |  |  |
| Roller brush 4" + tray | No. | 3 |  |  |
| 4 inch paint brush | No. | 3 |  |  |
| 3 inch paint brush | No. | 3 |  |  |
| 4" galvanised FC nails @100Pcs/Pkt | Kg | 35 |  |  |
| 3" galv nails @ 100Pcs/Pkt | Kg | 15 |  |  |
| 2" x 3.15mm bullet head galvanised nail @ 100Pcs/Pkt | Kg | 10 |  |  |
| 1" x 3.15mm clout galvanised nail @ 100Pcs/Pkt | Kg | 5 |  |  |
| 2.5" roofing twisted nail complete rubber washer | Kg | 25 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **Vat** |  |  |  |  |
| **other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. ***Mwaneaban Abaiang - seawall maintenance Project***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Material list for Mwaneaban Abaiang seawall maintenance Project at Betio.** | | |  | |
| **Description** | **Unit** | **Quantity** | **Price Quotation** | **T/Price Quotation** |
| Cement 40Kg | Bags | 152 |  |  |
| Sand | m³ | 7 |  |  |
| Gravel | m³ | 4 |  |  |
| Sandbags | Pcs | 88 |  |  |
| Shovels | No. | 15 |  |  |
| Wheelbarrow | No. | 3 |  |  |
| Gloves | Prs | 20 |  |  |
| Safety glasses | No. | 20 |  |  |
| Rubber boot | Prs | 20 |  |  |
| Vest | No. | 20 |  |  |
| Helmet | No. | 20 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **VAT** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

3.KUC Buota Residential House Material

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Material list for KUC Buota Residential House Material.** | | |  | |
| **Description** | **Unit** | **Qty for 1 Project** | **Price Quotation** | **T/Price Quotation** |
| 100x50mm timber pine 6m long for framing and trusses | Length | 100 |  |  |
| 75x50mm timber pine 6m long for purlins | Length | 42 |  |  |
| 15feet Colorbond roofing sheet | Sheet | 30 |  |  |
| 12feet Colorbond roofing sheet | Sheet | 30 |  |  |
| 9feet Colorbond roofing sheet | Sheet | 42 |  |  |
| 8feet Colorbond roofing sheet | Sheet | 30 |  |  |
| 8 blade louvre frame black | Prs | 30 |  |  |
| 6 blade louvre frame black | Prs | 2 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **VAT** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

4. Kuuma Church Butaritari Project

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for Kuuma Church Project at Butaritari island** | |  |  |  |
| **Description** | **unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Portland cement 40 Kg | Bags | 16 |  |  |
| Formply | Sheet | 6 |  |  |
| Nail 4" | Kilo | 8 |  |  |
| Nail 2" | Kilo | 2 |  |  |
| Reinf. rod 16mm dia | No. | 10 |  |  |
| Reinf. rod 6mm | No. | 9 |  |  |
| Tire wire | Roll | 1 |  |  |
| Pine timber 8x2x6mtr | Length | 24 |  |  |
| Pine timber 2x2x6mtr | Length | 3 |  |  |
| Nail 3" | Kg | 3 |  |  |
| Construction Plywood 1/4" | Sheets | 18 |  |  |
| Panel Pin | Kg | 5 |  |  |
| Varnish 4ltr | Tin | 12 |  |  |
| Golden Oak 4ltr | Tin | 6 |  |  |
| Hand brush 4" | No. | 18 |  |  |
| Roller Brush with tray | No. | 15 |  |  |
| Mouse Roller with tray | No. | 18 |  |  |
| Acrylic undercoat 4ltr | Tin | 37 |  |  |
| Semi-Gloss 4ltr | Tin | 37 |  |  |
| Wall putty | Bags | 6 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **VAT** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

1. Special School Bikenibeu - New Mass concrete seawall Project

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for special school new mass concrete seawall project at Bikenibeu** | |  |  |  |
| **Description** | **Unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Portland cement 40 Kg | Bags | 1,374. |  |  |
| Sands | m³ | 18 |  |  |
| Gravel | m³ | 36 |  |  |
| Backfill materials | m³ | 349 |  |  |
| Geotextile | Rollers | 3 |  |  |
| Sandbags | Bags | 1,874 |  |  |
| Formply sheets 3/4" | Sheet | 14 |  |  |
| Timber 100x50mm | Length | 22 |  |  |
| Nail 4" | Kg | 7 |  |  |
| Nail 3" | Kg | 4 |  |  |
| Nail 1 1/2" flat head | Kg | 3 |  |  |
| PVC pipe 100mm dia. | Length | 2 |  |  |
| Tape measure 50 mtr | No. | 1` |  |  |
| Tape measure 8 mtr | No. | 1 |  |  |
| Hand saw | No. | 2 |  |  |
| Crowbar | No. | 1 |  |  |
| Claw hammer | No. | 8 |  |  |
| Shovels | No. | 10 |  |  |
| Wheelbarrow | No. | 2 |  |  |
| Gloves | Prs | 21 |  |  |
| Safety glasses | No. | 21 |  |  |
| Rubber boot | Prs | 10 |  |  |
| Vest | No. | 21 |  |  |
| Helmet | No. | 21 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **Vat** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

6. St Iotebwa - New Mass concrete seawall

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for St Iotebwa new mass concrete seawall Project.** | |  |  |  |
| **Description** | **unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Portland cement 40 Kg | Bags | **550** |  |  |
| Sands | m³ | **5** |  |  |
| Gravel | m³ | **10** |  |  |
| Backfill materials | m³ | **91** |  |  |
| Geotextile | m² | **176** |  |  |
| Sandbags | Pcs | 788 |  |  |
| Formply sheets 3/4" | Sheet | 4 |  |  |
| Timber 100x50mm | Length | 22 |  |  |
| Nail 4" | Kg | 7 |  |  |
| Nail 3" | Kg | 4 |  |  |
| Nail 1 1/2" flat head | Kg | 3 |  |  |
| Tape measure 50 mtr | No. | 1` |  |  |
| Tape measure 8 mtr | No. | 1 |  |  |
| Hand saw | No. | 4 |  |  |
| Crow bar | No. | 2 |  |  |
| Claw hammer | No. | 4 |  |  |
| Shovels | No. | 10 |  |  |
| Wheel barrow | No. | 2 |  |  |
| Gloves | Prs | 21 |  |  |
| Safety glasses | No. | 21 |  |  |
| Rubber boot | Prs | 21 |  |  |
| PVC Pipe | No. | 2 |  |  |
| Helmet | No. | 21 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **VAT** |  |  |  |  |
| **Other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |

7.Taunibong Primary school

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for special school new mass concrete seawall Project at Bikenibeu** | |  |  |  |
| Description | Unit | Qty | Price Quotation | T/Price Quotation |
| Timber 2x2 | Length | 16 |  |  |
| Timber 3x2 | Length | 12 |  |  |
| Timber 6x2 | Length | 75 |  |  |
| Timber 8x2 | Length | 13 |  |  |
| Formply black | sheet | 10 |  |  |
| Roofing 15ft (sheets) | sheet | 33 |  |  |
| Roofing 12ft (sheets) | Sheet | 58 |  |  |
| Ridge COP (8”) | Length | 20 |  |  |
| Porland cement 40Kg | Bags | 231 |  |  |
| Rod D16 (For Pad foofing) | Length | 81 |  |  |
| Rod D10 | Length | 25 |  |  |
| Tire wire | Roll | 2 |  |  |
| Polythene 60 meter | Roll | 1 |  |  |
| Mesh Wire 200mm x 200mm SL72 | Sheet | 5 |  |  |
| Total cost |  |  |  |  |
|  |  |  |  |  |
| VAT |  |  |  |  |
| Other charges if any |  |  |  |  |
| Total cost (vat inclusive) |  |  |  |  |

1. ***Ueen te Rotario - New Mass Concrete seawall***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for special schoolnew mass concrete seawall Project at Bikenibeu** | |  |  |  |
| **Description** | **unit** | **Qty** | **Price Quotation** | **T/Price Quotation** |
| Portland cement 40 Kg | Bags | 450 |  |  |
| Sands | m³ | 5 |  |  |
| Gravel | m³ | 9 |  |  |
| Backfill materials | m³ | 78 |  |  |
| Geotextile | m3 | 142 |  |  |
| sandBags | Bags | 630 |  |  |
| Formply Sheets 3/4" | Sheet | 3 |  |  |
| Timber 100x50mm | Length | 22 |  |  |
| Nail 4" | Kg | 7 |  |  |
| Nail 3" | Kg | 4 |  |  |
| Nail 1 1/2" flat head | Kg | 3 |  |  |
| PVC pipe 100mm dia. | Length | 2 |  |  |
| Tape measure 50 mtr | No. | 1` |  |  |
| Tape measure 8 mtr | No. | 2 |  |  |
| Hand saw | No. | 2 |  |  |
| Crow bar | No. | 3 |  |  |
| Claw hammer | No. | 5 |  |  |
| Shovels | No. | 15 |  |  |
| Wheel barrow | No. | 3 |  |  |
| Gloves | Prs | 20 |  |  |
| Safety glasses | No. | 20 |  |  |
| Rubber boot | Prs | 10 |  |  |
| Helmet | No. | 20 |  |  |
| **Total cost** |  |  |  |  |
|  |  |  |  |  |
| **Vat** |  |  |  |  |
| **other charges if any** |  |  |  |  |
| **Total cost (vat inclusive)** |  |  |  |  |