**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **21-G016-24**

## Specification

### Background

The project aims to improve mobility of the Oceanic Fisheries Division’s Monitoring, Control and Surveillance (MCS) team. The need for procuring a vehicle to assist with transportation for port monitoring and inspections is essential to carry out duties required by fisheries inspectors and fisheries observers daily. The procurement of a vehicle can help for to effectively and efficient work by fisheries officers and observers.

### Requirements

The Ministry of Fisheries and Marine Resources Division through the Oceanic Fisheries Division requesting for quotations for sourcing of 1 Toyota Hilux 4x4 Double Cab with Manual Transmission and powered by Diesel that can accommodate at least 4 fisheries officers including a back carrier for equipment.

Note: Please a Detailed Specification of Double Cab should be also included in bid submission

### Installation services

Inclusion of

1. Warranty for 1 year.
2. Provision of spare parts.

### Delivery Time

It is anticipated that the goods can be delivered after 2 months of signing of contract.

## Description of the Goods

| **4WD-Vehicle** | **Supplier**  *(Specify the specifications provided in the Column "Offered Specifications", and comment any deviation from "Purchaser Requirements" in the Column "Comments on deviations")* | |
| --- | --- | --- |
| **Purchaser Requirements** | **Offered Specifications (to be filled out by the Supplier with detailed information)** | **Comments (to be filled out by the Supplier explaining any deviation)** |
| **Standard production vehicle of latest design in current production & supplied new** | **Latest generation Hiliux model** |  |
| **Designated to comply with heavy duty condition, suitable for operation in humid, tropical, coastal climate and in rough terrain.** | **Designed as a work truck for all climates and conditions.**  **Suitable for Kiribati condition.** |  |
| Designated for passengers and goods transport over unpaved ( rough) roads | 4WD Pickup Truck for both on and off road |  |
| **Seating capacity : min 5** | **5 Seats** |  |
| Number of doors: 4 | 4 doors |  |
| **Dimensions** |  |  |
| Overall length -4800 Mm +- 500 mm | 5330mm |  |
| Overall Width -4800 Mm +- 500 mm | **1855mm** |  |
| Overall Height -1800 Mm +- 200mm | 1815mm |  |
| Ground Clearance: 170-210 mm | **217mm** |  |
| Wheelbase: 3000+-200mm | 3085mm |  |
| Gross Vehicle Weight: Max. 3,000 kg | **2860KG** |  |
| **Engine** | 2GD-FTV |  |
| **5 cylinder** | **4 cylinder** |  |
| piston displacement-between 2000-3200cmcubic | 2400cc |  |
| **Transmission** |  |  |
| Manual | 6 Speed Manual |  |
| Selectable 2WD/4WD | **Easy knob selection** |  |
| Brakes and Tyres |  |  |
| Brakes -Front Ventilated disc brakes | Comes standard |  |
| Full size spare tyre with external lockable  All terrain tyres required for Kiritimati | 265/65/R17 |  |
| **Fuel** |  |  |
| Diesel | **DIESEL** |  |
| Fuel consumption/100Km | **7.1L/100KM Average** |  |
| Fuel capacity | **80L** |  |
| **Body and Equipment** |  |  |
| Exterior colour | **White** |  |
| fabric seating | **Fabric** |  |
| Seat-belts, front and rear | **Front and rear seat belt** | **For 5 passengers** |
| air conditioning | **Air conditioning with 5 air flow direction** |  |
| dual air bags | **Driver and passenger airbag** |  |
| Towing hook, front and rear | **Comes standard** |  |
| Corrosion protected panels-fender covers ( front) | **Comes standard** |  |
| Tray liner | **Not included** | **optional** |
| Tray cover – tonneau or other | **Not included** | **optional** |
| Green rating |  |  |
| Safety rating | **5 Start Australia ANCAP** |  |
| Warranty and Services | **Offered** |  |
| Full Manufactures Warranty -minimum 12 months or 20,000 kms- whichever should come first. | **2 Year Or 60,000KM**  **Whichever comes first** |  |
| Documentation and availability of spare parts, including comprehensive list of Spare parts held in stock including maintenance and technical support | **See attached list** |  |
| User's manual in the English language plus inspection booklet | **Comes with vehicle** |  |