**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **RFQ- 21-G007-24**

## Specification

### Background

The project aims to provide support for the purchase of the MFMRD transports, as in grave need to aid the Ministry operations. The Ministry continues to prioritize the well-being and operational efficiency of its workforce; hence the procurement of new office vehicles emerges as a strategic initiative to enhance employee mobility and support the overall organization operations.

### Recently, the Ministry implemented the use of private buses for transporting staff members to and from work. Unfortunately, there have been reports of dissatisfaction and unreliability with the service. It is also important that the Ministry implement this project to minimize costs of maintenance and transport hire as the current office vehicles remaining to be malfunctional. The Ministry plan to buy new vehicles that will support MFMRD activities and to address the workforce punctuality for effective and efficient delivery of service.

The project has gone through the DCC approval for procurement of 4 brand new office vehicles equipped with necessary features to meet the Ministry operational requirements. The 2 Buses will be used for official Ministry staff transport and for other official purposes such as commuting between offices (Betio KSVA, Bairiki HQ, Ambo and Tanaea Hatchery and Workshop). The 2 Four-Wheel Drive Hilux will cater for necessary fieldworks, attending meetings and transporting goods or equipment as needed. The specification for the vehicles is defined considering safety standards, fuel efficiency criteria and other relevant considerations such as the Ministry workforce to support runs across the Ministry divisions residing across the island.

To ensure the project aim is achieved, the Ministry working closely with the Procurement Office to facilitate this procurement of supply of the vehicles and also wish to seek quotation from suppliers on the 4 brand new vehicles with details and specification as clearly specified in the specifications below.

### Requirements

### Kindly refer to RFQ Evaluation criteria and method template for the criteria used.

### Also, please refer to RFQ Instruction on how to submit the Quotation part II -“Quotation Documents Required to be Submitted”. Page 5-6

### Including the following certificate- Cover letter, Certified Business registration certificate, Valid business license, and tax clearance document, technical and financial components.

* Provide of Quotation based on the landed cost (inclusive of CIF and other local charges) also mention if VAT inclusive

### Installation services

Inclusion of

1. Warranty Certificate for a period of 2 years.
2. Provision of spare parts.

### Delivery Time

After awarding of contract to the winning bidder, in 2 months it is expected for the project to be completed with these buses to be ready and delivered to MFMRD.

## Description of the Goods

**1. MINIBUS (TOYOTA HIACE COMMUTER)**

| **Photo of preferred vehicle.** |  | |
| --- | --- | --- |
| **4WD-Vehicle** | **Supplier**  *(Specify the specifications provided in the Column "Offered Specifications", and comment any deviation from "Purchaser Requirements" in the Column "Comments on deviations")* | |
| **Purchaser Requirements** | Offered Specifications (to be filled out by the Supplier with detailed information) | Comments (to be filled out by the Supplier explaining any deviation) |
| **Standard production vehicle of latest design in current production & supplied new** | Standard production vehicle of latest design in current production & supplied new |  |
| **Designated to comply with heavy duty condition, suitable for operation in humid, tropical, coastal climate and in rough terrain.** | Designed as a transport for all climates and conditions.  Suitable for Kiribati condition. |  |
| Designated for passengers and goods transport over unpaved (rough) roads | Standard mini bus |  |
| **SEATING CAPACITY: min 16** | 12-16 seats |  |
| Number of doors: | 3 doors (with the boot at the rear end of the bus) |  |
| **DIMENSIONS** |  |  |
| Overall length -4800 Mm +- 500 mm | 4695 mm |  |
| Overall Width -4800 Mm +- 500 mm | 1695 mm |  |
| Overall Height -1800 Mm +- 200mm | 1980 mm | - |
| Ground Clearance: 170-210 mm | 185 mm |  |
| Wheelbase: 3000+-200mm | 2570 mm |  |
| Gross Vehicle Weight: Max. 3,000 kg | Curb weight: 1850 kg  2,950 kg |  |
| **ENGINE** | 2.8L turbo diesel engine |  |
| **cylinder** | 4 cylinders |  |
| **piston displacement** | Between 2000-3200cm cubic |  |
| **TRANSMISSION** |  |  |
| **Manual** | 6-speed manual  Horsepower: 142 hp |  |
| **Selectable 2WD/4WD** |  |  |
| **BRAKES AND TYRES** |  |  |
| Brakes | **Front ventilated disc brakes** |  |
| Tyres | Full size spare tyre with external lockable |  |
| **FUEL** |  |  |
| Diesel | **Diesel** |  |
| Fuel consumption | **7.5 L per 100km to 8.5 L per 100 km.** |  |
| Fuel capacity | **70L** |  |
| **BODY AND EQUIPMENT** |  |  |
| Exterior colour | **White** |  |
| fabric seating | **Fabric** |  |
| Seat-belts | **Front and rear seat belt included** |  |
| Air conditioning | **Air conditioning with 5 air flow direction** |  |
| dual air bags | **Driver and passenger airbag** |  |
| Towing hook, front and rear | **Comes standard** |  |
| Corrosion protected panels-fender covers ( front) | **Comes standard** |  |
| Tray liner | **Not included** | **optional** |
| Tray cover – tonneau or other | **Not included** | **optional** |
| Green rating | **Low emissions** |  |
| Safety rating | **5 Star Australia ANCAP** |  |
| Warranty and Services | **Period of 2 year** |  |
| Full Manufactures Warranty -minimum 12 months or 20,000 kms- whichever should come first. | **2 Year Or 60,000KM**  **Whichever comes first** |  |
| Inclusion of documentation and availability of spare parts, including comprehensive list of Spare parts held in stock including maintenance and technical support | **Provided documentation and list of spare parts, including maintenance and technical support.** |  |
| User's manual in the English language plus inspection booklet | **Comes with vehicle** |  |

**2.BIG BUS - NEW TOYOTA COASTER (seat 29)**

| **Photo of preferred vehicle.** | C:\Users\Moanibou Ngaruenga\Downloads\Screenshot 2024-04-04 at 17-08-31 Sales Quotation - TOYOTA COASTER 4.2D MT.pdf.png | |
| --- | --- | --- |
| **4WD-Vehicle** | **Supplier**  *(Specify the specifications provided in the Column "Offered Specifications", and comment any deviation from "Purchaser Requirements" in the Column "Comments on deviations")* | |
| **Purchaser Requirements** | Offered Specifications (to be filled out by the Supplier with detailed information) | Comments (to be filled out by the Supplier explaining any deviation) |
| **Standard production vehicle of latest design in current production & supplied new** | Standard production vehicle of latest design in current production & supplied new |  |
| **Designated to comply with heavy duty condition, suitable for operation in humid, tropical, coastal climate and in rough terrain.** | Designed as a transport for all climates and conditions.  Suitable for Kiribati condition. |  |
| Designated for passengers and goods transport over unpaved (rough) roads | Standard |  |
| **SEATING CAPACITY: min 29** | 29 seats |  |
| Number of doors: | 2 doors (driver and passenger) |  |
| **DIMENSIONS** |  |  |
| Overall length | 6000mm - 7500mm |  |
| Overall Width | 2000 mm – 3500mm |  |
| Overall Height | 2300mm - 3500 mm | - |
| Ground Clearance: | As appropriate |  |
| Wheelbase: 3000+-200mm | 2570 mm |  |
| Gross Vehicle Weight: |  |  |
| **ENGINE** | 2.8L turbo diesel engine |  |
| **cylinder** | 4 cylinders |  |
| **piston displacement** |  |  |
| **TRANSMISSION** |  |  |
| **Manual** | 6-speed manual |  |
| **Selectable 2WD/4WD** | **Any as appropriate** |  |
| **BRAKES AND TYRES** |  |  |
| Brakes |  |  |
| Full size spare tyre with external lockable |  |  |
| **FUEL** |  |  |
| Diesel | **Diesel** |  |
| Fuel consumption/100Km |  |  |
| Fuel capacity |  |  |
| **BODY AND EQUIPMENT** |  |  |
| Exterior colour | **White** |  |
| fabric seating | **Fabric** |  |
| Seat-belts, front and rear | **Front and rear seat belt** |  |
| air conditioning | **Air conditioning with 5 air flow direction** |  |
| dual air bags | **Driver and passenger airbag** |  |
| Towing hook, front and rear | **Comes standard** |  |
| Corrosion protected panels-fender covers ( front) | **Comes standard** |  |
| Tray liner | **Not included** | **optional** |
| Tray cover – tonneau or other | **Not included** | **optional** |
| Green rating |  |  |
| Safety rating | **5 Star Australia ANCAP** |  |
| Warranty and Services | **Offered** |  |
| Full Manufactures Warranty -minimum 12 months or 20,000 kms- whichever should come first. | **2 Year Or 60,000KM**  **Whichever comes first** |  |
| Documentation and availability of spare parts, including comprehensive list of Spare parts held in stock including maintenance and technical support | **Provided documentation with spare parts including maintenance and technical support.** |  |
| User's manual in the English language plus inspection booklet | **Comes with vehicle** |  |

**3. BRAND NEW TOYOTA HILUX WORKMATE (4×4 CAR SEAT) – QUANTITY 2**

| **Photo of preferred vehicle.** |  | |
| --- | --- | --- |
| **4WD-Vehicle** | **Supplier**  *(Specify the specifications provided in the Column "Offered Specifications", and comment any deviation from "Purchaser Requirements" in the Column "Comments on deviations")* | |
| **Purchaser Requirements** | Offered Specifications (to be filled out by the Supplier with detailed information) | Comments (to be filled out by the Supplier explaining any deviation) |
| **Standard production vehicle of latest design in current production & supplied new** | Latest generation Hilux model |  |
| **Designated to comply with heavy duty condition, suitable for operation in humid, tropical, coastal climate and in rough terrain.** | Designed as a work truck for all climates and conditions.  Suitable for Kiribati condition. |  |
| Designated for passengers and goods transport over unpaved ( rough) roads | 4WD Pickup Truck for both on and off road |  |
| **Seating capacity : min 5** | 5 Seats |  |
| Number of doors: 4 | 4 doors |  |
| **Dimensions** |  |  |
| Overall length -4800 Mm +- 500 mm | 5330mm |  |
| Overall Width -4800 Mm +- 500 mm | 1855mm |  |
| Overall Height -1800 Mm +- 200mm | 1815mm |  |
| Ground Clearance: 170-210 mm | 217mm |  |
| Wheelbase: 3000+-200mm | 3085mm |  |
| Gross Vehicle Weight: Max. 3,000 kg | 2860KG |  |
| **Engine** | 2GD-FTV |  |
| cylinder | 4 cylinder |  |
| piston displacement-between 2000-3200cmcubic | 2400cc |  |
| **Transmission** |  |  |
| Manual | 6 Speed Manual |  |
| Selectable 2WD/4WD | **Easy knob selection** |  |
| **B**rakes and Tyres |  |  |
| Brakes -Front Ventilated disc brakes | Comes standard |  |
| Full size spare tyre with external lockable | 265/65/R17 |  |
| **Fuel** |  |  |
| Diesel | **DIESEL** |  |
| Fuel consumption/100Km | **7.1L/100KM Average** |  |
| Fuel capacity | **80L** |  |
| **Body and Equipment** |  |  |
| Exterior colour | **1 white and 1 grey** |  |
| fabric seating | **Fabric** |  |
| Seat-belts, front and rear | **Front and rear seat belt** | **For 5 passengers** |
| air conditioning | **Air conditioning with 5 air flow direction** |  |
| dual air bags | **Driver and passenger airbag** |  |
| Towing hook, front and rear | **Comes standard** |  |
| Corrosion protected panels-fender covers ( front) | **Comes standard** |  |
| Tray liner | **Not included** | **optional** |
| Tray cover – tonneau or other | **Not included** | **optional** |
| Green rating |  |  |
| Safety rating | **5 Star Australia ANCAP** |  |
| Warranty and Services | **Offered** |  |
| Full Manufactures Warranty -minimum 12 months or 20,000 kms- whichever should come first. | **2 Year Or 60,000KM**  **Whichever comes first** |  |
| Documentation and availability of spare parts, including comprehensive list of Spare parts held in stock including maintenance and technical support | **Provided documentation with spare parts, including maintenance and technical support.** |  |
| User's manual in the English language plus inspection booklet | **Comes with vehicle** |  |