**REQUEST FOR QUOTATION  
SPECIFICATION OF GOODS**

**Procurement No:** **RFQ-43-G014-24**

## Specification

### Background

The purpose of this tender is to seek a CIF price in AUD local currency from any Registered Supplier willing to furnish a 20-foot container with 50 sets of flexi-tanks. This procurement will be carried out over a two-year period under a framework agreement. Further details or specs for the flexi-tank and other attachments are provided below:

**Quantity: in a 20ft Container**

50 Sets of Flexi tanks

50 Rolls of Corrugated Papers

50 Pcs of Cardboards

1. Pcs of Press Foam Strips

02 PLTS of 100 pcs Frame Bulkheads

* **Flexi tank Information & Specification:**

1. Flexi tank Serial Number – 240211041442
2. Flexi tank Model / Name – 24CBM Bottom Fill / Discharge Flexi tank
3. Flexi tank Nominal Volume Capacity – 24,000 Litre
4. Flexi tank number of Layers – 5 as detailed and tabulated below,

|  |  |  |  |
| --- | --- | --- | --- |
| ***5 layers for a flexi tank*** | ***Material*** | ***Thickness*** | ***Weight / sq meter*** |
| Layer 1 | PP | 334micron | 170gsm |
| Layer 2 | PE | 125micron | 115gsm |
| Layer 3 | PE | 125micron | 115gsm |
| Layer 4 | PE | 125micron | 115gsm |
| Layer 5 | PE | 125micron | 115gsm |

* **Valve Configuration: (***Bottom Fixed with Flexi tank***)**

|  |  |  |  |
| --- | --- | --- | --- |
| ***Valve Type*** | ***Model Number*** | ***Design*** | ***Size*** |
| Bottom | 104001 | 3” Butterfly Camlock Valve | 3” |
| Air Vent / Relief | N/A | N/A | N/A |

* **Bulkhead Specification:** 
  + - * + Bulkhead Type – Adjustable Frame Bulkhead
        + Two-piece welded gate carbon steel

### Flexitanks are liquid bulk material flexible storage containers that are primarily used by KCDL in the packaging of finished copra crude oil (CNO) for exporting purposes. Therefore, in order to maintain KCDL's continuous operation through CNO exporting, it is critical to ensure that these tanks are available at all times and must be ordered at least 7-8 times per year.

### Requirements

All supporting documentation must be in English. The following supporting documents should be provided

1. Business Registration with nature of business indication that the tenderer is capable to order Flexi tanks in bulk. Failure to provide such registration will result in disqualification of the tenderer. This is applicable only for international Tenderers
2. Signed certificate for compliance form should be provided. (Failure will result in disqualifying the tenderer)
3. Valid business license from the relevant Councils
4. Tax clearance letter from Tax Office for tax registered companies (Failure to provide will result in rejection of the tender)
5. Bank statement (To ensure the companies have their financial capacity to do the procurement, this requirement should be provided. Failure to provide will result in the disqualification of the tender)
6. A complete quotation for financial component of the proposal
7. A complete technical requirement in achieving the specifications of goods indicated in this “Specification template”

### Installation services

Not applicable

### Delivery Time

Every consecutive two months a year for a period of two years’ agreement.

## Description of the Goods

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | 50 sets of flexi tank in one Container | 7-8 orders | Every consecutive two months a year | $ |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |