**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** 15-G003-25

## Specification

### Background

The project was proposed from Aranuka Island Council to help better equipped the island with multi-purpose workshop. This project will accommodate the islanders need by providing more opportunities and to maintaining transports on Aranuka. The island council promised that this project will ensure positively development and improvement to the livelihood of the islander through employment creation and revenue generated.

### Requirements

All supporting documentation must be in English. Not that the list of requirement can be found in the **Instruction on** **How to submit Tender** refer to page 5

### Installation services

* Construction Services

### Delivery Time

The suppliers are required to provide the delivery time frame & plan.

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | 40 kg Portland cement | 228 |  |  |
| 2 | Sand | 8 |  |  |
| 3 | Aggregate | 32 |  |  |
| 4 | Formply 2.0x1.2 per sheet | 12 |  |  |
| 5 | Pine Timber 150x25mm in Length | 5 |  |  |
| 6 | Pine Timber 50x50mm in length | 8 |  |  |
| 7 | Polthene 50x50mm in length | 9 |  |  |
| 8 | Arc Fabric mesh wire 5.5mx2.13m (59m2) | 8 |  |  |
| 9 | Rod 10mm dia. Reinfrocing bar in 6m length | 44 |  |  |
| 10 | Rod 12mm dia. Reinforcing bar in 6m length | 27 |  |  |
| 11 | Rod 6mm dia. Reinforcing bar in 6m length | 51 |  |  |
| 12 | 200mm block | 922 |  |  |
| 13 | 100x4 galv metal strap (30m/roll) | 1 |  |  |
| 14 | 10 blade louver frame | 3 |  |  |
| 15 | 4 blade louver frame | 4 |  |  |
| 16 | 75x50mm timber pine | 23 |  |  |
| 17 | 50x50mm timber pine | 6 |  |  |
| 18 | 200x25mm fascia board & barge board | 10 |  |  |
| 19 | 100x50mm timber pine | 25 |  |  |
| 20 | 150x25mm timber pine | 2 |  |  |
| 21 | 100x50mm dressed dakua for header, mullion and door frame and window | 11 |  |  |
| 22 | 150x50mm dakua for window sill | 2 |  |  |
| 23 | Masonite hardboard lining 2.4x1.2 | 4 |  |  |
| 24 | 12mm plywood for gusset | 5 |  |  |
| 25 | Corrugated zincalum roof decking |  |  |  |
| 26 | 17ft zincalum roofing | 40 |  |  |
| 27 | Alum ridge capping @ 2.4m/pcs | 6 |  |  |
| 28 | Alum fascia gutter @ 2.4m/pcs | 11 |  |  |
| 29 | Gutter bracket 1.2m | 11 |  |  |
| 30 | Stop ends joint to gutter | 4 |  |  |
| 31 | 100mm dia vent cowl | 1 |  |  |
| 32 | 100mm diameter pvc downpipe and vent | 2 |  |  |
| 33 | 100mm diameter bend | 2 |  |  |
| 34 | 100mm tee | 1 |  |  |
| 35 | Gutter outlet 100mm dia | 2 |  |  |
| 36 | Blind rivert 4.6mm @ 100no/pkt | 2 |  |  |
| 37 | Silicone sealant | 2 |  |  |
| 38 | Standard flush door 40x400x200mm | 1 |  |  |
| 39 | Standard flush door 40x800x200mm hung in pairs | 1 |  |  |
| 40 | 100mm butt brass hinges | 6 |  |  |
| 41 | Night latch lock complete with handles and keys | 2 |  |  |
| 42 | 100mm barrel bolt complete with screw | 2 |  |  |
| 43 | Pvc pipe 15mm distribution line | 3 |  |  |
| 44 | Elbow pvc 15mm | 7 |  |  |
| 45 | Male adaptor 15mm | 1 |  |  |
| 46 | Female adaptor 15mm | 1 |  |  |
| 47 | Pilla tap 15mm | 1 |  |  |
| 48 | Thead tape | 2 |  |  |
| 49 | Solvent cement 500g | 1 |  |  |
| 50 | 4’0” LED light fitting complete | 4 |  |  |
| 51 | Light switch one way | 2 |  |  |
| 52 | Light switch two way | 1 |  |  |
| 53 | 1.5mm cable wire | 48 |  |  |
| 54 | Mounting block | 6 |  |  |
| 55 | Insulating tape | 2 |  |  |
| 56 | Double power point | 2 |  |  |
| 57 | Switch board complete with circuit breaker, wiring and connect | 1 |  |  |
| 58 | Wall plug | 2 |  |  |
| 59 | Pink primer 4 litres | 1 |  |  |
| 60 | Acrylic Undercoat 4 litres | 3 |  |  |
| 61 | Semi Gloss 4 litres | 3 |  |  |
| 62 | Tray complete with roller and sleeve | 3 |  |  |
| 63 | 3” paint brush | 2 |  |  |
| 64 | 2” paint brush | 2 |  |  |
| 65 | 4” galvanised nail | 26 |  |  |
| 66 | 3” galvanised nail | 5 |  |  |
| 67 | 2” galvanised nail flat head | 4 |  |  |
| 68 | 3” twisted roof nail with rubber | 4 |  |  |
| 69 | 12mm dial Bolts & nuts | 25 |  |  |
| 70 | Panel pin | 1 |  |  |
| 71 | Cement 40kg | 40 |  |  |
| 72 | 200mm bricks | 128 |  |  |
| 73 | F62 Fabric mesh wire 6mx2.4m/sheet | 1 |  |  |
| 74 | Rod 12mm diameter 6m | 11 |  |  |
| 75 | Rod 6mm diameter 6m | 5 |  |  |
| 76 | Tie wire (45m/roll) | 10 |  |  |
| 77 | 100L water tank | 1 |  |  |
| 78 | Shovel | 4 |  |  |
| 79 | Wheel barrows | 2 |  |  |
| 80 | Colt cutter | 1 |  |  |
| 81 | Crow bars | 1 |  |  |
| 82 | Trowel 200mm pointed | 2 |  |  |
| 83 | Trowel plaster | 2 |  |  |
| 84 | Circular saw | 1 |  |  |
| 85 | Block mould 200mm thick | 1 |  |  |
| 86 | Cordless drill | 1 |  |  |
| 87 | Leadwire 20m | 1 |  |  |
| 88 | Angle grinder | 1 |  |  |
| 89 | Hose 12mm dimeter 25 | 1 |  |  |
| 90 | Silicone gun | 1 |  |  |
| 91 | Rivet gun | 1 |  |  |
|  |  |  |  |  |