**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **47-G009-25**

## Specification

### Background

The Kiribati Ports Authority is looking to procure 1 high Shelving for heavy-duty warehouse tasks, and narrow aisle operation

### Requirements

All supporting documentation must be in English.

Refer template 2

### Installation services

None

### Delivery Time

1-2 months after payment is completed

## Description of the Goods

|  |  |
| --- | --- |
| Preferred Brand & Model | Heli - CDD16-950 |
| Load Capacity | 1,600 kg |
| Lift Height | Up to 5.8 m |
| Power Supply | Electric (24V) |
| Battery Options | Lead-acid 280Ah or Lithium 200Ah |
| Operator Position | Walkie |
| Fork Size | 1,150 mm × 550 mm |
| Overall Width | 957 mm |
| Overall Length | 2,105 – 2,525 mm |
| Turning Radius | 1,595 – 2,010 mm |
| Safety Features | Electronic power steering, regenerative braking, emergency reversing device, curve automatic deceleration, high position automatic speed reduction |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | Shelving Stacker | 1 | 1-2 month |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |

*Note: Specification and minimum requirements of good is on the evaluation criteria template*